{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Base_MiniCentrale"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Base_MiniCentrale","index":0,"n_rows":107,"n_cols":378,"rows_kept":107,"cut":false,"hidden":false,"merged":[]}
[]
["Num_quest","COD_QUARTIER_VILLAGE_HAMEAU","Date","Reg","Dep","Com","Localite","Nb_Men","Population","Anne_Pop","Date_mise_serv","Date Arrêt MC","Nbre Heure Fonc MC","Nom_Oper","Nom_Progrmme","Nb_N1","Nb_N2","Nb_N3","Nb_N4","Nb_ab_Tot","Personn_contac","Num_pers_con","Niv_Qualif_Cond","For_Cond","Contr_Op","Mont_Rem_Cond","Retar_payement","Coord_X","Coord_Y","Typ_MC","Fonct_MC","Emplac_ter","Statu_Jur_Ter","Exist_Clot","Dim_Ter_L1_C1 : Col1","Dim_Ter_L1_C1 : Col2","Dim_Ter_L2_C1 : Col1","Dim_Ter_L2_C1 : Col2","Dim_Ter_L3_C1 : Col1","Dim_Ter_L3_C1 : Col2","Pos_ext_Ter","Natur_Clot","Nat_port_Clot","Porte_1","Porte_2","Mur_pot_1","Mur_pot_2","Poteaux_Grillage_1","Poteaux_Grillage_2","Rep_Cloture","Rep_Poteaux_Grillage","Rep_port","Rep_port_Autre","Long_Tech_Long","Larg_Tech_Long","Ext_Loc_Ond","Mur_loc_tec_1","Mur_loc_tec_2","Toit_loc_tec_1","Toit_loc_tec_2","Port_loc_tec_1","Port_loc_tec_2","Fenetre_loc_tec_1","Fenetre_loc_tec_2","peinture_loc_tec_1","peinture_loc_tec_2","Plancher_loc_tec_1","Plancher_loc_tec_2","Mur_loc_rep","Toit_rep","port_rep","Fenetre_rep","peint_Rep","Plancher_rep","Long_Loc_Tec","Lar_Loc_Tec","Haut_Loc_Tec","Aer_Loc_Ond_1","Aer_Loc_Ond_2","Plancher_1","Plancher_2","Mur_1","Mur_2","Toiture_1","Toiture_2","Loc_Ond_Porte_1","Loc_Ond_Porte_2","fenetre_1","fenetre_2","Peinture_1","Peinture_2","Ventilation_1","Ventilation_2","Rep_loc_Ond_Aer","Rep_loc_Ond_Planch","Rep_loc_Ond_Mur","Rep_loc_Ond_Toit","Rep_loc_Ond_Port","Rep_loc_Ond_Fenêt","Rep_loc_Ond_Peint","Rep_loc_Ond__Vent","Natur_ond_1","Natur_ond_2","Typ_Ond_Charg","Typ_Ond_reseau","Marq_ond_Charg","Marq_ond_reseau","Nbr_Ond_Char : Col1","Nbr_Ond_Char : Col2","Puis_Ond_Char : Col1","Puis_Ond_Char : Col2","Tableau2_L1_C1 : Col1","Tableau2_L1_C1 : Col2","Tableau2_L2_C1 : Col1","Tableau2_L2_C1 : Col2","Tableau2_L3_C1 : Col1","Tableau2_L3_C1 : Col2","Tableau2_L4_C1 : Col1","Tableau2_L4_C1 : Col2","Heure du relevé  : Col1","Heure du relevé  : Col2","Car_Ondu_L1_C1 : Col1","Car_Ondu_L1_C1 : Col2","Car_Ondu_L1_C1 : Col3","Car_Ondu_L1_C1 : Col4","Car_Ondu_L2_C1 : Col1","Car_Ondu_L2_C1 : Col2","Car_Ondu_L2_C1 : Col3","Car_Ondu_L2_C1 : Col4","Car_Ondu_L3_C1 : Col1","Car_Ondu_L3_C1 : Col2","Car_Ondu_L3_C1 : Col3","Car_Ondu_L3_C1 : Col4","Car_Ondu_L4_C1 : Col1","Car_Ondu_L4_C1 : Col2","Car_Ondu_L4_C1 : Col3","Car_Ondu_L4_C1 : Col4","Fonc_Charg_1","Fonc_Charg_2","Fonc_Reseau_1","Fonc_Reseau_2","Pos_Aug_Ond","Comb_Nb_Ond","Dat_Rempl_Ond_Charg","Dat_Rempl_Ond_Reseau","Long_Loc_Bat","Lar_Loc_Bat","Haut_Loc_Bat","Etat_Mur_1","Etat_Mur_2","Etat_Toiture_1","Etat_Toiture_2","Etat_Porte_1","Etat_Porte_2","Etat_Fenaitre_1","Etat_Fenaitre_2","Etat_Peintur_1","Etat_Peintur_2","Etat_Plancher_1","Etat_Plancher_2","Etat_Aeration_1","Etat_Aeration_2","Etat_Vent_1","Etat_Vent_2","Rep_Loc_Bat_Mur","Rep_Loc_Bat_Toit","Rep_Loc_Bat_Porte","Rep_Loc_Bat_Fenetre","Rep_Loc_Bat_Peinture","Rep_Loc_Bat_Plancher","Rep_Loc_Bat_Aeration","Rep_Loc_Bat_Ventilation","Ligne_3","Ligne_4","Nb_bat","Tens_sys_Stock","Car_Tens","Car_Cap","Car_Temp_Max","Car_Temp_Min","Etat_bat_L2_C1","Etat_bat_L3_C1","Etat_bat_L5_C1","Temp_ambiante","Temp_batterie","Ni_Electrolyte","Dat_Remp_Batt","heur_rel_don_bat","Cable_Bat","Fusible_Bat","Coss_Bat","Fonct_Batt","Long_Loc_GE","Lar_Loc_GE","Hauteur_Loc_GE","Aer_loc_GE_1","Aer_loc_GE_2","Etat_Toit_GE_1","Etat_Toit_GE_2","Etat_plan_GE_1","Etat_plan_GE_2","Etat_des_murs_GE_1","Etat_des_murs_GE_2","Etat_des_portes_GE_1","Etat_des_portes_GE_2","Etat_des_fenetres_Ge_1","Etat_des_fenetres_Ge_2","Etat_Vent_GE_1","Etat_Vent_GE_2","Rep_Aer_GE","Rep_Toit_GE","Rep_Plancher_GE","Rep_Mur_Ge","Rep_Portes_GE","Rep_Fenetre_GE","Rep_Vent_GE","Etat_cab_Ge","Marq_Ge","Dat_mis_Ser_GE","Etat_Fonc_GE","Si_Nf_quand","Nb_heur_Fon_GE","Puissance_GE","Frequence_Ge","Tension_GE","Pression_huile_bar_GE","Temperature_eau_GE","Niveau_carburant_GE","Tension_Batterie_GE","Cap_batterie_Dem","Car_GE_Puis","Car_GE_Tens","Car_GE_Frequence","Car_GE_PRP_Puis","Car_Tens_Bat_Dem","Car_cap_Bat_Dem","Car_GE_Mono_Triphase","Ligne_1","Ligne_7","Typ_dem_GE","Resr_mere","Cap_res_mer","apr_centr","Nb_apr_car","Qute_ap","Nb_heur_fonc","Pan_GE","Si_oui_Typ_Pann","Nb_Heur_moy_Insd","Dat_Rempl_GE","Puissance_Champ_PV","Nb_Champ","Nb_Mod","Nom_Fabric","Ref_mod","Tech_Panneaux","Puis_Cret_mod","Cour_op_mod","Tension_optimale_Mod","Tension_Circuit_Ouvert_Mod","Courant_Court-circuit_Mod","Sup_bet_PV_1","Sup_bet_PV_2","Sup_str_met_PV_1","Sup_str_met_PV_2","Etat_surface_1","Etat_surface_2","Cablage_PV_1","Cablage_PV_2","Boite_Jonction_PV_1","Boite_Jonction_PV_2","Mis_ter_PV_1","Mis_ter_PV_2","Parafoudr_PV_1","Parafoudr_PV_2","Omb_por_PV_1","Omb_por_PV_2","Nb_mod_rep","Nb_cab","Nb_sup_struc_met","Nb_par","Tens_glob_sor_mod","Ensoleillement","heur_lec_ten_dc","Dat_Rem_Mod","Nat_Pot","Typ_Lum","Etat_cabl_res_dis_1","Etat_cabl_res_dis_2","Etat_acces_enc_res_dis_1","Etat_acces_enc_res_dis_2","Pot_acces_enc_res_dis_1","Pot_acces_enc_res_dis_2","Ep_Acces_enc_res_dis_1","Ep_Acces_enc_res_dis_2","Nb_Cabl_RD","Ligne_2","Acces_encra_RD","Manchon_de_jonction_RD","Capot_dextremite_BT_RD","Mise_a_la_terre_RD","Nb_pot_RD","Nb_EP_Pub","Nb_Pot_rep","Ec_pub_L1_C1","Foy_lim_L1_C2","Porte_RD","Long_Reseux","Nb_poteaux","Typ_cable_1","Typ_cable_2","Observ","Entre_Gen_PV","Entret_Ond","Entre_Sys_Stockage","Entr_GE","Installation_Interieure","Resp_Entr_Gen_Pv","Resp_Entr_Ond","Res_Entr_Sys_de_Sto","GE","Rsp_Entr_Inst_Int","Ass_Entr_Gen_Pv1_1","Ass_Entr_Gen_Pv1_2","Ass_Entr_Gen_Pv1_3","Ass_Entr_Ond1_1","Ass_Entr_Ond1_2","Ass_Entr_Ond1_3","Ass_Entr_Sys_de_Sto1_1","Ass_Entr_Sys_de_Sto1_2","Ass_Entr_Sys_de_Sto1_3","Ass_Ent_GE_1","Ass_Ent_GE_2","Ass_Ent_GE_3","Ass_Entr_Inst_Int_1","Ass_Entr_Inst_Int_2","Ass_Entr_Inst_Int_3","Dure_moy_Int_Gen_Pv2","Dure_moy_Int__Ond2","Dure_moy_Int__Sys_de_Sto2","Dure_moy_Int_GE1","Dure_moy_Int_Int1","Int_Pan_Gen_Pv3_1","Int_Pan_Gen_Pv3_2","Int_Pan_Gen_Pv3_3","Int_Pan_Ond3_1","Int_Pan_Ond3_2","Int_Pan_Ond3_3","Int_Pan_Sys_de_Sto3_1","Int_Pan_Sys_de_Sto3_2","Int_Pan_Sys_de_Sto3_3","Int_PanGE2_1","Int_PanGE2_2","Int_PanGE2_3","Int_Pan_Inst_Int1_1","Int_Pan_Inst_Int1_2","Int_Pan_Inst_Int1_3","Dur_Int_Gen_Pv2","Dur_Int_Ond2","Dur_Int_Sys_de_Sto2","Dur_Int_PanGE1","Dur_Int_Inst_Int","Resg_Suiv_Mc","Ligne_5","Ligne_6","Systeme_de_Stockage","GE1","Installation_Interieure1","Mod_PV_Def","Ond_Def","Bat_Def","Inst_Int_Def","SystSock_Dech","Comment_Sckag_dech","Sys_dest_Dechet","Sys_trait_dechet","Syst_traitement","Obser"]
["P2","1412020200700","12/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","SONKO KOUNDA",65,1250,2020,"01/01/2011","01/08/2013",0,"NS RESIF","ERSEN I",11,4,10,7,32,"DJIBA MANE",785406984,"CULTIVATEUR","Non","Oui",10000,"Non",406942,1427934,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",18.5,null,16.600000000000001,null,1.83,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,38,null,null,null,5.73,2.86,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,null,"REMPLACER SERRURES DES LOCAUX  ONDULEURS BATTERIE ET GE",null,"RAFRAICHIR LA PEINTURE",null,2.5299999999999998,1.78,3.16,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"PRESENCE DE TROUS","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4,{"$nulls":11},48,null,550,null,null,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2012",null,3.49,2.5499999999999998,3.13,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE DE TROUS","REMPLACER LA SERRURE","RAFRAICHIR LA PEINTURE",null,null,null,"PAS DE VENTILATION","8 OPZ S800","HOPPECK",24,48,2,800,{"$nulls":4},22,30,null,null,null,"16:27","Bon Etat","Mauvais Etat","Bon Etat","Mauvais Etat",2.79,2.1,2.78,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"RAFRAICHIR LA PEINTURE","RAFRAICHIR LA PEINTURE",null,"PAS DE VENTILATION","Mauvais","CUMMINS","01/01/2011","Non Fonctionnel","27/08/2013",{"$nulls":9},11,400,50,{"$nulls":5},"BATTERIE DECONNECTE","Manuel","Non",null,"Oui",4,20,2,"Oui",null,null,null,5,3,12,"EL SOLAR","ET P636 140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A réparer","Bon",null,"Mauvais","A réparer","Bon",null,"Bon",{"$nulls":6},14,null,null,"Bois","LBC","Mauvais","A réparer","Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A réparer",4,{"$nulls":4},3,12,1,5,6,1,42,342,47,"3*35","4*16",null,4,null,3,null,null,"Oui",null,"Oui",null,null,"Conducteur",{"$nulls":5},"Conducteur",{"$nulls":8},2,null,1,{"$nulls":5},"Opérateur",{"$nulls":5},"Opérateur",null,null,"Opérateur",null,null,null,2,null,2,3,"Non","Non","Non","Non","Non","Non",null,2,null,1,"Non"]
["P3","1412010400300","22/07/2020","SEDHIOU","SEDHIOU","KOUSSY","BARY",27,660,2019,"01/01/2015",0,9,"Sud Solar System","ERSEN II",19,4,1,4,28,"KEBA DRAME",774695374,"CULTIVATEUR","Non","Non",10000,"Oui",428473,1422798,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.64,null,17.899999999999999,null,2.2200000000000002,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},7.48,2.85,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer",{"$nulls":5},"PLUSIEURS FISSURES",2.73,2.5,2.95,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4,45,261,1.74,3,229,229,{"$nulls":5},48,null,750,null,null,null,22,null,230,220,240,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"remplacer la serrure",{"$nulls":4},"pas de ventilation","90 pz s SOLAR POWER 1370","HOPPECKE",21,42,2,1370,null,null,86,null,44,31,35,"Bas",null,"18:26","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.76,2.7,2.77,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Bon","CUMMINS",{"$nulls":12},22,400,50,{"$nulls":4},"G22 D5",{"$nulls":12},5,1,22,"CANADIAN SOLAR","CS 6 P 230P","Mono",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Mauvais",{"$nulls":5},263,13,"17:26",null,"Bois","LBC","Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":7},2,0,null,6,1,32,130,14,"3*35","4*16","REMPLACER 6 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35",4,4,3,null,null,"Oui","Oui","Oui",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":8},2,10,1,{"$nulls":8},"Opérateur",{"$nulls":5},"Opérateur",{"$nulls":4},40,null,3,"Non","Non","Non","Non","Non","Non",null,null,3,null,"Non"]
["P4","1412030102800","22/07/2020","SEDHIOU","SEDHIOU","BAMBALI","SORANGE",48,650,2020,"01/01/2013",0,11,"NS RESIF","ERSEN II",27,4,2,0,33,"BASSIROU A DIATTA",782599456,"TAILLEUR","Non","Oui",10000,"Non",428941,1399639,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18.41,null,16.18,null,1.62,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",44,5,null,null,7.5,2.86,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",{"$nulls":6},"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE PAR ENDROIT",2.7,2.4700000000000002,2.81,"Mauvais Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"DEGRADATION PAR ENDROIT",{"$nulls":5},"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4,55,305,6,8.3000000000000007,230,230,{"$nulls":5},48,null,550,null,null,20,22,null,230,230,null,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2018",null,4.21,2.4700000000000002,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,null,"presence de trou",null,null,"rafraichir la peinture","degradation par endroit",null,"pas de ventilation","10 opz s 1000","HOPPECKE",23,46,2,1000,null,null,null,1250,54,28,30,"Equilibré",null,"12:47","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.74,2.73,2.66,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"INFILTRATION EAU",null,null,null,"INFILTRATION EAU QUAND IL YA DU VENT",null,"Bon","GREEN POWER GP 22",null,"Fonctionnel",{"$nulls":8},11,null,null,240,50,15,12,100,null,"GP 22 SH PW A","MF DIN 100","Manuel","Non",null,"Oui",null,40,2,"Oui","TABLEAU AFFICHAGE",4,null,5,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},350,31,"11:47",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",{"$nulls":7},2,null,3,3,40,81,24,"3*35","4*16","REMPLACER 18 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X 35mm2. PREVOIR UN CONTRE FICHE OU 2 POTEAUX JUMELEES POUR UNE FIN DE LIGNE",2,2,2,3,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,5,1,40,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":6},1,null,3,null,"Non","Non","Non","Non","Non","Non",null,1,null,null,"Non",{"$nulls":4},"UNEBATTERIE LAISSEE DANS LE LOCAL BATTERIE"]
["P5","1422030103700","21/07/2020","SEDHIOU","BOUNKELING","DIAROUME","SOUAKI",64,997,2019,"01/01/2013","01/01/2013",0,"NS RESIF","ERSEN II",4,16,7,2,29,"BASSAF DAFE\nBASSAF DAFFE",777209121,"CULTIVATEUR","Non","Non",null,null,417737,1430940,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",18.36,16.899999999999999,16.899999999999999,null,1.94,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,1,"Autre","RAFRAICHIR LA PEINTURE",7.48,5.78,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état",{"$nulls":6},"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.73,2.52,3.2,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER SERRURE",null,null,"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4,null,309,{"$nulls":9},48,null,750,null,null,null,22,null,230,220,240,null,50,50,60,"Non Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.17,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","90 PZS SOLAR POWER 1370","HOPPECKE",24,48,2,1370,{"$nulls":4},46,27,null,"Haut","01/01/2017","18:57","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.94,2.93,2.84,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Bon","CUMMINS",null,"Fonctionnel",{"$nulls":10},22,400,50,{"$nulls":4},"C 22 D5",null,"Manuel","Non",null,"Oui",null,40,null,"Non",null,null,null,5,1,22,"CANADIAN SOLAR","CS 6 P 230 P","Mono",230,7.78,29.6,3608,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},323,2,"18:10",null,null,null,"Bon",null,"Bon",null,"A remplacer",null,"A remplacer",{"$nulls":6},1,1,2,null,6,2,45,400,32,"3*35","4*16","REMPLACER 17 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2 . METTRE UN CONTRE FICHE OU 2 POTEAUX JUMELEES POUR UNE FIN DE LIGNE",{"$nulls":33},"Opérateur",null,null,"Opérateur",{"$nulls":13},"Non","Non","Non","Non","Non","Non",null,1,null,null,"Non",{"$nulls":4},"PAS DE REPONSES A CERTAINES QUESTIONS CAR LE CONDUCTEUR EST INJOIGNABLE ET L'ANCIEN SUPERVISEUR DE L'OPERATEUR EST DECEDE"]
["P6","1412010200300","21/07/2020","SEDHIOU","SEDHIOU","SAKAR","BANY",56,1227,2020,"01/01/2010",0,3,"Sud Solar System","ERSEN II",9,9,6,6,30,"AHMADOU BAMBA DRAME",776116876,"CULTIVATEUR","Non","Non",10000,null,454536,1420361,"Solaire_GE","Oui","Inondable","Non Immatriculé","Oui",17.5,null,17.3,null,1.73,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,10,"Autre",null,7.55,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,null,null,"REMPLACER SERRURES LOCAUX ONDULEUR ET BATTERIE",null,null,"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.77,2.5499999999999998,3.17,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":7},"REMPLACER SERRURE",null,"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4,null,349,{"$nulls":9},48,null,750,null,null,null,22,null,230,220,240,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2018",null,4.24,2.5099999999999998,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE D'UNE FISSURE","REMPLACER SERRURE",null,"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","10 OPZ S 1000","HOPPECKE",20,40,2,1000,{"$nulls":4},32,29,null,"Equilibré",null,"11:47","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.95,2.9,2.81,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","Bon","GREEN POWER","01/01/2010","Fonctionnel",null,null,null,52.8,241,null,58,{"$nulls":4},240,50,15,12,72,null,"GP 22 SH PW A","SMF DIN 75","Manuel","Non",null,"Oui",1,30,3,"Oui","SYSTEME INJECTION",1440,null,5,1,22,"CANADIAN SOLAR","CS 6 P 230P","Mono",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Mauvais",null,1,null,null,null,325,13,"10:52","01/01/2017",null,null,"Bon",null,"Bon",null,"A réparer",null,"A remplacer",{"$nulls":8},1,1,7,1,812,38,28,"3*35","4*16","REMPLACER 23 PORTEES DE 4X 16mm2 PAR UN CABLE DE 3X35mm2 . PREVOIR UN CONTRE FICHE OU 2 POTEAUX JUMELEES POUR UNE FIN DE LIGNE",3,3,3,3,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},2,2,2,2,2,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Sous traitant",null,null,"Opérateur",null,null,10,7,30,1,7,"Non","Non","Non","Non","Non","Non",null,null,11,null,"Non",{"$nulls":4},"4 BATTERIES LAISSEES DANS LE LOCAL BATTERIE"]
["P7","1412010200100","20/07/2020","SEDHIOU","SEDHIOU","SAKAR","BABADI",75,830,2019,"01/01/2011","01/01/2018",0,"Sud Solar System","ERSEN II",18,4,2,9,33,"MADJIRA SOLY",773166259,"CULTIVATEUR","Non","Non",10000,"Non",445790,1421356,"Solaire_GE","Non","Inondable","Délibération","Oui",18.600000000000001,null,16.899999999999999,null,1.8,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer",null,7,"Autre",null,7.5,5.0750000000000002,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer",{"$nulls":5},"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.72,2.46,2.91,"Mauvais Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",{"$nulls":4},"CHEMIN CABLE DE TERRE",{"$nulls":4},"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4,48,320,1.27,1.9,230,230,{"$nulls":5},48,null,550,null,null,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2016",null,4.0250000000000004,2.048,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"INFILTRATION LATERALE D'EAU",{"$nulls":4},"PAS DE VENTILATION","10OPZS 1000","HOPPECK",22,44,2,1000,null,null,null,1280,32,27,30,"Bas",null,"17:04","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.85,2.9,2.65,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":8},"INFILTRATION LATERALE D'EAU",null,"Bon","GREEN POWER","01/01/2011","Fonctionnel",{"$nulls":11},240,50,15,12,75,null,"GP 22 SH/ PW A","CMF 57512 DIN 72","Manuel",null,null,"Oui",1,20,2,"Non",null,null,null,5,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",{"$nulls":5},379,5,"16:12",null,"Bois","LBC","A remplacer",null,"A remplacer",null,"A réparer",null,"Bon",null,28,16,1,1,null,1,null,null,1,3,5,27,202,22,"3*35","4*16","REMPLACER 15 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2 . PREVOIR UN CONTRE FICHE OU 2 POTEAUX JUMELEES POUR UNE FIN DE LIGNE",6,4,3,null,null,"Oui","Oui","Oui",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":8},2,20,15,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":5},"Opérateur",null,null,7,4,2,null,10,"Non","Non","Non","Non","Non","Non",null,null,6,null,"Non"]
["P8","1412020101400","18/07/2020","SEDHIOU","SEDHIOU","Bemet Bidjini","FRANCOUNDA BADJI COUNDA",34,905,2020,"01/12/2012","2020-04-01",0,"NS RESIF","ERSEN II",0,16,11,null,27,"IBRAHIMA GASSAMA",778682670,"CULTIVATEUR","Non","Oui",10000,"Oui",402489,1405930,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",17.34,null,16.95,null,1.8,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Bon Etat",null,20,null,"pomelle",null,7.43,5.76,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,null,"PRESENCE DE FISSURES ET TROUS","REMPLACER SERRURE LOCAL ONDULEUR",null,"RAFRAICHIR LA PEINTURE",null,2.71,2.4700000000000002,null,"Mauvais Etat",null,"A réparer",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":6},"PRESENCE DE FISSURE","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,5,null,355,{"$nulls":9},48,null,550,null,null,null,230,null,23020,22,null,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2017",null,4.21,2.4500000000000002,3.15,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":5},"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","100PZS 1000","HOPPECKE",19,38,2,1000,null,null,null,1244,36,26,null,"Equilibré",null,"18:50","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.61,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE FISSURE",null,null,null,"INFILTRATIONS LATERALES D'EAU","PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/12/2012","Fonctionnel",null,null,null,53,242,null,86,{"$nulls":4},240,50,15,2,75,null,"GP 22 SH / PW A","MF DIN 75","Manuel","Non",null,"Oui",1,30,4,"Oui","PROBLEME DE CABLAGE . BATTERIE GE DEFECTUEUSE",720,null,5,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},357,5,"18:07",null,"Bois","LBC","Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A remplacer","Bon",null,45,16,1,1,null,null,2,null,1,8,null,45,400,34,"3*35","4*16","REMPLACER 12 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",1,4,1,2,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},2,2,2,2,2,"Opérateur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,2,45,15,null,"Non","Non","Non","Non","Non","Non",null,null,24,null,"Non",{"$nulls":4},"6 BATTERIES DEFECTUEUSES DANS LE LOCAL BATTERIE"]
["P9","1412010200200","20/07/2020","SEDHIOU","SEDHIOU","SAKAR","BANDOUGA",70,1200,2019,"01/01/2012",0,3,"Sud Solar System","ERSEN II",24,12,6,4,46,"LAMINE THIAM",776603196,"TAILLEUR","Non","Non",10000,null,436575,1413856,"Solaire_GE","Oui","Inondable","Non Immatriculé","Oui",18.420000000000002,null,16.7,null,2.2000000000000002,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",7,5,null,null,7.5,5,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer",null,"PRESENCE DE TROUS",null,null,null,"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.74,2.5,3.21,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER SERRURE",null,null,"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4,null,344,{"$nulls":9},48,null,750,21.7,56,null,22,null,230,220,20,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,2.4900000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",{"$nulls":4},"PAS DE VENTILATION","90 PZ S SOLAR POWER 1370","HOPPECKE",24,48,2,1370,{"$nulls":4},29,29,null,"Bas",null,"11:00","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.74,2.72,2.5499999999999998,"Bon Etat",null,"Mauvais Etat","A réparer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE TROU","QUELQUES DEGRADATIONS",null,null,"INFILTRATIONS LATERALES D'EAU","PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2012","Fonctionnel",null,368.1,null,52.3,233,4.9000000000000004,59,67,14.1,null,null,240,50,15,12,75,null,"GP 22 SH/PW N A","DIN 75","Manuel","Non",null,"Oui",1,30,3,"Non",null,4488,null,5,1,22,"CANADIAN SOLAR","CS 6P 230P","Mono",230,7.78,29.6,36.299999999999997,8.34,"Bon",null,"Bon",null,"Mauvais","A remplacer",null,null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,1,null,null,null,366,12,"09:58",null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"Mauvais","A remplacer",{"$nulls":7},7,1,0,7,34,68,34,"3*35","4*16","REMPLACER 23 PORTEES DE 4X16mm2PAR UN CABLE DE 3 X35 mm2",10,15,15,15,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,10,10,30,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":8},6,4,4,null,null,"Non","Non","Non","Non","Non","Non",1,null,24,null,"Non"]
["P10","1412010102000","19/07/2020","SEDHIOU","SEDHIOU","DIENDE","SALIKEGNE",58,946,2020,"01/01/2013","2018-01-01",0,"Sud Solar System","ERSEN II",34,1,2,3,40,"FODE DRAME",775258640,"MILITAIRE A LA RETRAITE","Non","Oui",20000,"Oui",428471,1422802,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",18.399999999999999,null,17,null,1.8,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},7.5,5.69,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",{"$nulls":5},"RAFRAICHIR PEINTURE PARTIE EXTERNE MUR","DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.5,2.5,3.17,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":47},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":25},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",null,null,null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":12},"01/01/2013","Non Fonctionnel",{"$nulls":22},"Oui",null,80,{"$nulls":66},"4 POTEAUX EN FER ONT DES LAMPADAIRES FONCTIONNELS . PASSAGE DU RESEAU HYBRIDE AU RESEAU DE LA SENELEC"]
["P11","1412010100800","19/07/2020","SEDHIOU","SEDHIOU","DIENDE","DIATOUMA",86,1474,20203,"04/07/2014",0,5,"Sud Solar System","ERSEN II",22,null,2,2,26,"BOURAMA DEMBA",779458822,"CULTIVATEUR","Non","Non",5000,null,436625,1413871,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.600000000000001,34.9,16.8,16.8,1.97,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",35,3,"pomelle",null,7.5,2.88,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",{"$nulls":5},"RAFRAICHIR PEINTURE PARTIE EXTERNE DU MUR","PRESENCE DE FISSURES",2.5,2.74,2.9,"Mauvais Etat","A Remplacer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER SERRURE",null,null,"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,5,null,337,{"$nulls":9},48,null,550,21.7,56,20,22,null,230,null,230,null,50,50,60,"Non Fonctionnel",null,"Fonctionnel",null,"Non",null,null,"01/01/2018",3.2,2.5,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",{"$nulls":4},"PAS DE VENTILATION","90PZS SOLAR POWER 1370","HOPPECKE",21,42,2,1370,{"$nulls":4},37,30,null,"Equilibré","01/11/2019","15:14","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.75,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"RAFRAICHIR LA PEINTURE",null,"INFILTRATIONS LATERALES D'EAU","PAS DE VENTILATION","Bon","CUMMINS","04/07/2014","Fonctionnel",{"$nulls":10},22,400,50,null,12,100,null,"C 22D5","DIN 100SMF","Manuel","Non",null,"Oui",1,20,4,"Oui","PROBLEME DE DEMARRAGE",720,null,5,1,22,"CANADIAN SOLAR","CS 6 P 230 P","Mono",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",null,null,"Bon",null,1,null,null,null,337,12,"14:24",null,"Bois","LBC","Bon",null,"A remplacer",null,"A remplacer","A réparer","A remplacer",null,null,null,1,null,null,null,2,1,3,3,7,50,150,29,"3*35","4*16","REMPLACER 22 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",4,4,4,4,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,30,20,20,{"$nulls":4},"Opérateur",{"$nulls":8},"Opérateur",{"$nulls":6},3,"Non","Non","Non","Non","Non","Non",null,1,3,null,"Non"]
["P12","1412010100600","19/07/2020","SEDHIOU","SEDHIOU","DIENDE","BISSARY DIOUNKOUA",67,1215,2019,"07/12/2014",0,4,"Sud Solar System","ERSEN II",25,10,3,2,40,"DOUDOU FIKOU",772694602,"MACON","Non","Non",5000,"Non",402463,1405660,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.5,null,17.45,null,1.95,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,4,null,null,null,7.5,2.85,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",{"$nulls":6},"COURONNE DE PROTECTION PERIPHERIQUE",2.2000000000000002,2.46,3.3,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4,48,285,3.18,15.5,230,230,{"$nulls":5},48,null,750,21.7,56,null,22,null,230,220,240,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":8},"PAS DE VENTILATION","90PZS SOLAR POWER 1370","HOPPECKE",20,40,2,1370,null,null,100,1230,50,26,31,"Bas",null,"11:21","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.73,2.67,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Bon","CUMMINS","01/01/2015","Fonctionnel",{"$nulls":8},13,null,22,400,50,null,12,100,null,"C22 D5","NS 100","Manuel","Non",null,"Oui",1,30,2,"Oui","PROBLEME DE VIDANGE. DE FIL DE TERRE  . DE CABLE",1440,null,5,1,22,"CANADIAN SOLAR","CS 6P 230P","Mono",230,7.78,29.6,36.799999999999997,8.36,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,1,null,null,null,285,20,"10:04",null,"Bois","LBC","A remplacer",null,"A remplacer",null,"A remplacer","A réparer","Mauvais","A remplacer",49,16,1,1,null,null,2,5,4,6,5,49,545,52,"3*35","4*16","REMPLACER 41 PORTEES DE 4X16mm2 PAR UN CABLE DE 3 X35mm2",5,4,5,4,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},35,4,10,30,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,7,4,1,5,2,"Non","Non","Non","Non","Non","Non",1,null,6,null,"Non",{"$nulls":4},"2 BATTERIES ET 1 LAMPADAIRE LAISSE DANS LE LOCAL BATTERIE"]
["P13","1412020101500","18/07/2020","SEDHIOU","SEDHIOU","Bemet Bidjini","FRANCOUNDA SARAKHOLE",58,1111,2019,"01/01/2010","01/06/2013",0,"NS RESIF","ERSEN I",7,10,10,5,32,"BOURAMA DIAWARA",773020622,"CULTIVATEUR","Non","Non",10000,"Non",397886,1401082,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",20.350000000000001,null,15.2,null,1.97,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":5},5.68,5.73,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",{"$nulls":5},"RAFRAICHIR LA PEINTURE PARTIE EXTERNE DU MUR","FISSURES AU NIVEAU DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.4700000000000002,1.72,3.6,"Mauvais Etat","A Remplacer","A réparer",null,"Mauvais Etat","A réparer","A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":4},"REPARER CHEMIN DE CABLE",null,"PRESENCE D'UN TROU","REMPLACER SERRUR",null,"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION",{"$nulls":7},5,{"$nulls":13},48,null,null,null,30,150,265,{"$nulls":6},50,null,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2012","01/01/2012",3.43,2.4900000000000002,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"TROUS ET FISSURES","REMPLACER SERRURE",null,"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","80PZS800","HOPPECK",24,48,2,800,{"$nulls":4},22,27,null,"Bas",null,"15:55","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.72,1.95,2.46,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE TROUS",null,null,"RAFRAICHIR LA PEINTURE",null,null,"Bon","CUMMINS","01/01/2010","Fonctionnel","01/01/2013",{"$nulls":9},11,400,50,{"$nulls":4},"C11D5",null,"Manuel",null,null,"Oui",2,40,1,"Non",null,null,null,5,3,12,"SOLAR","ET P63 6140","Mono",140,7.95,17.600000000000001,21.96,8.41,"A réparer",null,"Bon",null,"Bon",null,"Mauvais",null,"Bon",null,"A réparer",null,null,null,"Bon",{"$nulls":5},74,7,"15:28",null,"Bois","LBC","Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A remplacer","A remplacer",null,269,35,20,1,null,null,18,3,null,4,3,44,389,30,"3*35","4*16","REMPLACER 19 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",3,1,4,3,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,10,40,30,{"$nulls":4},"Opérateur",{"$nulls":8},"Opérateur",null,null,null,2,null,null,4,"Non","Non","Non","Non","Non","Non",null,1,24,null,"Non"]
["P14","1412020101800","18/07/2020","SEDHIOU","SEDHIOU","Bemet Bidjini","sibikoroto 2",56,1005,2020,"01/01/2010","01/01/2015",0,"NS RESIF","ERSEN I",23,5,2,3,33,"abdou seydi",772243239,"cultivateur","Non","Oui",10000,"Non",419865,1413362,"Solaire_GE","Non","Inondable","Délibération","Oui",15.5,null,15.3,null,1.67,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Bon Etat",null,null,null,"pomelle",null,5.67,2.81,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",{"$nulls":5},"RAFRAICHIR PEINTURE PARTIE EXTERNE DU MUR","QUELQUES FISSURES AU NIVEAU DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.46,1.68,3.15,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"A réparer",{"$nulls":6},"PRESENCE DE FISSURE ET DE TROUS","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION",{"$nulls":36},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.42,2.4500000000000002,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat",null,null,"PRESENCE DE TROU","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","80PZS 800","HOPPECK",23,46,2,800,{"$nulls":4},68,30,null,"Bas",null,"11:51","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,1.95,2.4900000000000002,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE FISSURES",null,"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","Mauvais","CUMMINS","01/01/2010","Non Fonctionnel","01/01/2017",{"$nulls":7},5,null,11,400,50,null,12,75,null,"C11D5","DIN 75","Manuel","Non",null,"Oui",null,40,1,"Oui","BATTERIE . PROBLEME DE CABLAGE",null,null,5,3,12,"SOLAR","ET P63 6140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais",null,null,null,"Mauvais",{"$nulls":5},70,6,"10:45",null,"Bois","LBC","Mauvais","A remplacer",null,null,"A remplacer",null,"Mauvais","A remplacer",180,35,9,5,null,null,10,null,1,9,1,45,435,33,"3*35","4*16","PREVOIR 2 POTEAUX POUR METTRE DES CONTRE FICHES . REMPLACER 8 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",4,6,3,2,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,5,30,5,{"$nulls":10},"Opérateur",null,null,"Opérateur",{"$nulls":5},2,3,"Non","Non","Non","Non","Non","Non",null,1,2,1,"Non"]
["P15","1412030201800","17/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","MADINA LINKETO",73,939,2018,"01/01/2010",0,6,"NS RESIF","ERSEN I",24,4,3,5,36,"ISMAELA BADIANE",785657954,"MEUNIER","Non","Oui",10000,"Oui",412169,1404869,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",20.100000000000001,null,15.1,null,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},5.7,2.83,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"RAFRAICHIR LA PEITURE PARTIE EXTERNE MUR",{"$nulls":4},"PRESENCE DE FISSURES SUR LA COURONNE DE PROTECTION PERIPHERIQUE",2.48,1.72,2.92,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",{"$nulls":9},"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,5,52,196,2.23,3.9,231,231,{"$nulls":5},48,null,550,null,21.7,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2013",null,3.42,2.4700000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":5},"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","90PZS SOLAR POWER 1370","HOPPECKE",23,46,2,1370,null,null,98,1300,52,28,31,"Bas","01/10/2019","16:00","Bon Etat","Bon Etat","Mauvais Etat","Bon Etat",1.96,2.73,2.75,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Mauvais","CUMMINS",null,"Non Fonctionnel","01/01/2012",{"$nulls":9},11,400,50,{"$nulls":4},"C11D5",null,"Automatique","Non",null,"Oui",1,20,2,"Oui","GE TOMBE EN PANNE SUITE A UNE TONNERE",null,null,5.04,3,12,"ET SOLAR","ET P636140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,"Bon",{"$nulls":5},200,8,"15:42",null,null,null,"Bon",null,"Bon",null,"A remplacer","A réparer",{"$nulls":7},1,3,5,1,0,5,44.5,100,52,"3*35","4*16",null,5,10,10,15,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},4,3,3,3,null,"Opérateur",{"$nulls":5},"Opérateur",{"$nulls":8},20,null,8,null,null,"Non","Non","Non","Non","Non","Non",null,null,1,null,"Non",{"$nulls":4},"18 BATTERIES LAISSEES DANS LE LOCAL BATTERIES (DECHETS)"]
["P16","1412030201300","17/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","karantaba linketo",72,1099,2019,"01/01/2015",0,4,"NS RESIF","ERSEN II",25,3,null,1,29,"PREVIA YANKATTE",772694690,"ENSEIGNANT","Non","Non",6000,"Non",413258,1407578,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.059999999999999,null,16.5,null,1.63,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,1,"Autre","RAFRAICHIR PEINTURE",7.6,6.05,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A réparer",{"$nulls":5},"DEGRADATION COURONNE DE PROTECTION PERIPHERIQUE",2.74,2.75,3.2,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":6},"PRESENCE DE TROUS ET DE FISSURES","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4.5999999999999996,40,323,4,3.5,230,230,{"$nulls":5},48,null,550,26.1,50,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2019",null,4.3,2.74,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE DE TROUS ET FISSURES","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","10 OPZS 1000","HOPPECKE",22,44,2,1000,null,null,null,1236,41,27,32,"Haut","01/01/2019","12:07","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.72,2.72,2.94,"Bon Etat",null,"Mauvais Etat","A réparer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"INFILTRATION D'EAU",{"$nulls":4},"PAS DE VENTILATION","Bon","GREEN POWER GP 22",null,"Fonctionnel","01/01/2019",{"$nulls":10},240,50,15,null,null,null,"GP22 SH /PW A",null,"Manuel","Non",null,"Oui",null,40,2,"Non","BATTERIE GE DETERIORE",3,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"A réparer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",{"$nulls":5},306,14,"10:55",null,"Bois",null,"Bon",null,"Bon",null,"A remplacer",null,"Mauvais","A remplacer",{"$nulls":6},1,11,null,0,11,40.200000000000003,1560.8,31,"3*35","4*16","17 PORTEES DE 4X16 mm2 A REMPLACER PAR UN CABLE DE 3X35mm2",8,10,10,10,null,"Oui","Oui","Oui",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},45,20,20,15,{"$nulls":4},"Opérateur",null,null,"Opérateur",{"$nulls":9},3,null,null,null,"Non","Oui","Oui","Oui","Oui","Oui",null,null,2,null,"Non",{"$nulls":4},"4 BATTERIES (DECHETS) LAISSEES DANS LE LOCAL BATTERIE"]
["P17","1412030202700","16/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","SINGHERE MANDING",120,1730,2020,"01/01/2014",0,5,"NS RESIF","ERSEN II",13,16,7,2,38,"LANDING KEITA",782132908,"CULTIVATEUR","Non","Oui",10000,"Oui",401097,1401383,"Solaire_GE","Oui","Inondable","Non Immatriculé","Oui",18.75,null,15.82,null,1.7,null,"Non","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",25.82,2,null,null,7.38,5.79,"Non","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",{"$nulls":6},"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.74,2.4900000000000002,2.9,"Mauvais Etat","A Remplacer","Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",{"$nulls":5},"PRESENCE DE FISSURES",null,null,null,"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4.5999999999999996,51,327,3,4.9000000000000004,230,230,{"$nulls":5},48,null,550,50,26.1,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2018",null,4.07,2.4700000000000002,2.94,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,null,"10 OPZS 1000","HOPPECKE",23,46,2,1000,{"$nulls":4},51,28,32,"Bas",null,"16:30","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.74,2.72,2.74,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":5},"PRESENCE DE PLUSIEURS TROUS ET FISSURES",{"$nulls":4},"Bon","GREN POWER GP 22",null,"Fonctionnel",null,null,null,53,240,null,77,{"$nulls":4},240,50,15,null,12,"100","GP 22 SH/PW A",null,"Manuel","Non",null,"Oui",1,40,1,"Non",null,720,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",{"$nulls":5},331,10,"16:20",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer",{"$nulls":5},1,2,10,1,0,10,50,350,48,"3*35","4*16","REMPLACER 19 PORTEES DE 4X 16mm2 PAR UN CABLE DE 3X35mm2",4,2,4,4,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,30,1,30,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":6},8,null,null,null,"Non","Non","Non","Non","Non","Non",null,null,1,null,"Non"]
["P18","1412030202600","16/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","SINGHERE BAYNOUCK",55,681,2019,"10/07/2011","23/08/2018",0,"NS RESIF","ERSEN I",7,12,4,null,23,"OMAR BIAYE",775258561,"CULTIVATEUR","Non","Oui",10000,"Oui",393778,1427999,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",20.98,26.78,10.47,15.57,2.1,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",31.45,1,null,null,5.7,5.71,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",{"$nulls":5},"RAFRAICHIR PEINTURE PARTIE EXTERNE DU MUR","FISSURES AU NIVEAU DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.46,1.73,3.19,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":6},"FISSURES SUR LA TOITURE","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","HP COMPACT 6000 - 48","HP COMPACT 6000 - 48",null,5,{"$nulls":13},48,48,{"$nulls":6},230,{"$nulls":4},50,null,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.44,2.46,3.2,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","8OPZS 800","HOPPECKE",15,30,2,800,{"$nulls":4},76,29,29,"Bas","01/01/2011","11:22","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.71,1.96,2.78,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE TROUS",{"$nulls":4},"PAS DE VENTILATION","Mauvais","CUMMINS",null,"Non Fonctionnel","01/08/2018",{"$nulls":9},11,400,50,{"$nulls":4},"C11 D5",null,"Manuel","Non",null,"Oui",1,20,3,"Oui",null,null,"01/08/2012",5.04,3,12,"ET SOLAR","ET P63 6140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,null,null,"Bon",null,1,null,null,null,78,23,"12:18",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer",{"$nulls":6},2,4,null,1,4,30.16,2000,25,"3*35","4*16",null,3,2,3,2,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Opérateur",null,null,20,5,2,1,20,{"$nulls":6},"Opérateur",null,null,"Opérateur",{"$nulls":7},1,2,null,"Non","Non","Non","Non","Non","Non",1,null,24,null,"Non"]
["P19","1412030102600","15/07/2020","SEDHIOU","SEDHIOU","BAMBALI","MISSIRA",46,970,2019,null,"01/01/2017",0,"NS RESIF","ERSEN II",6,30,10,null,46,"BACARY DIANKO",770484615,"FORGERON","Non","Oui",10000,"Oui",432072,1390661,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",17.72,null,17.2,null,1.83,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",42.92,6,null,null,7.53,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A réparer",null,null,"REMPLACER SERRURES LOCAUX BATTERIE ET ONDULEUR",null,null,"DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.64,2.5,3.6,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"A réparer",{"$nulls":6},"UNE PARTIE DE LA TOITURE EST ENLEVE PAR LE VENT",null,null,"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4.5999999999999996,45.6,237,null,null,229,229,{"$nulls":5},48,null,550,56,21.7,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.22,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE DE TROUS",null,"RAFRAICHIR LA PEINTURE",null,null,null,"PAS DE VENTILATION","10 OPZS 1000","HOPPECK",24,48,2,1000,null,null,19,null,45.6,29,30,"Bas",null,"19:30","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.74,2.72,2.86,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Bon","GREEN POWER GP 22",null,"Fonctionnel",{"$nulls":11},240,50,15,null,12,"70","GP 22SH / PW-A",null,"Automatique","Non",null,"Oui",1,70,3,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},360,4,"18:32",null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"Mauvais","A remplacer",{"$nulls":7},3,1,12,3,null,null,30,"3*35","4*16","remplacer 15 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",15,15,15,null,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",{"$nulls":5},1,1,1,1,{"$nulls":21},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non"]
["P20","1412030200700","15/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","BOUMOUDA SOUCOUTOTO",72,800,2020,"01/01/2010","15/03/2019",0,"NS RESIF","ERSEN II",4,11,8,null,23,"DEMBO MANE",773199756,"CULTIVATEUR","Non","Oui",10000,"Oui",399254,1396559,"Solaire_GE","Non","Inondable","Non Immatriculé","Oui",21.8,null,14.7,null,2.1,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,2,null,null,5.95,5.52,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,null,null,"CHANGER SERRURES LOCAUX ONDULEUR ET BATTERIE",null,"RAFRAICHIR PEINTURE PARTIE EXTERNE DU MUR","DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.5,1.72,2.89,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":7},"REMPLACER SERRURE",null,"RAFRAICHIR LA PEINTURE","PAS DE VENTILATION",{"$nulls":36},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.36,2.5,2.92,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","8 OPZS 800","HOPPECK",24,48,2,800,{"$nulls":4},39,34,null,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.76,1.98,2.85,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE TROUS",null,"RAFRAICHIR LA PEINTURE","RAFRAICHIR LA PEINTURE",null,"PAS DE VENTILATION","Bon","CUMMINS",null,"Non Fonctionnel","20/02/2020",{"$nulls":7},4,null,11,400,50,null,null,12,"72","C 11D5","MF DIN 72","Manuel","Non",null,"Oui",1,20,4,"Oui","RADIATEUR",3600,null,5.04,3,12,"ET SOLAR","ET P636140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais",null,"Bon",null,"Bon",{"$nulls":6},14,null,null,"Bois","LBC","Bon",null,"A remplacer",null,"Mauvais","A remplacer","Mauvais","A remplacer",null,null,4,null,null,1,7,15,null,0,15,45.1,135.30000000000001,28,"3*35","4*16","REMPLACER 14 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35 mm2",4,15,15,15,2,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Opérateur",null,null,30,5,20,10,{"$nulls":4},"Opérateur",{"$nulls":5},"Sous traitant",null,null,"Opérateur",{"$nulls":5},1,null,"Non","Non","Non","Non","Non","Non",null,1,null,null,"Non"]
["P21","1412030200600","15/07/2020","SEDHIOU","SEDHIOU","DJIREDJI","BOUMOUDA SOUCOTO",134,2005,2019,"01/01/2013",0,4,"NS RESIF","ERSEN I",4,16,13,1,34,"LANDING BADIO",772985016,"CULTIVATEUR","Non","Oui",10000,"Non",399595,1397845,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",19.12,null,16.52,null,1.64,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,3,"Autre","RAFRAICHIR PEINTURE",7.73,5.66,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer","A réparer",null,"Mauvais état","A remplacer",null,null,"REMPLACER SERRURE LOCAUX ONDULEUR ET BATTERIE",null,"RAFRAICHIR PEINTURE EXTERNE DU MUR","DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.73,2.48,3,"Mauvais Etat","A Remplacer","A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":4},"REPARER CHEMIN DE CABLE",null,null,"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4.5999999999999996,56,369,2.83,2.9,368,230,{"$nulls":5},48,null,550,50,26.1,20,22,null,230,null,230,{"$nulls":4},"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/07/2018",null,4.2,2.48,3.02,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"REMPLACER SERRURE",{"$nulls":4},"PAS DE VENTILATION","10 OPZS 1000","HOPPECK",24,48,2,1000,{"$nulls":4},56,32,32,"Bas","01/04/2020","11:00","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.72,2.72,2.76,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"RAFRAICHIR LA PEINTURE . PRESENCE DE FISSURES",null,null,"PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2013","Non Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GP 22 SH/PW-A",null,"Manuel","Non",null,"Oui",1,40,2,"Oui","FILTRAGE  POMPE",2880,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais",{"$nulls":5},345,13,"10:53",null,"Bois","LBC","Mauvais","A remplacer","Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer",33,16,null,null,null,2,1,3,null,5,3,33.380000000000003,null,32,"3*35","4*16","REMPLACER 24 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",2,2,2,2,2,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Opérateur",null,null,1,3,3,4,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,7,4,3,2,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non"]
["P22","1412030102400","14/07/2020","SEDHIOU","SEDHIOU","BAMBALI","MARON COUNDA",40,634,2020,"01/01/2015",0,12,"NS RESIF","ERSEN II",4,11,10,2,27,"MAMADOU MARON",773272479,"CULTIVATEUR","Non","Non",null,null,430625,1389913,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.18,null,16.940000000000001,null,2.0299999999999998,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,null,null,7.5,5.71,"Oui","A réparer",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,null,"TOITURE LOCAL BATTERIE EN TRES MAUVAIS ETAT","REMPLACER SERRURE LOCAL BATTERIE",null,"RAFRAICHIR PEINTURE PARTIE EXTERNE DU MUR","DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.7,2.4300000000000002,3.2,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER SERRURE",null,null,"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4.5999999999999996,52,167,1.55,1.44,231,231,{"$nulls":5},48,null,750,26.1,50,null,22,null,230,220,240,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2018",null,4.1500000000000004,2.4,3.16,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"UNE PARTIE DU TOITURE EST EMPORTEE PAR LE VENT",null,null,"RAFRAICHIR LA PEINTURE",null,null,"PAS DE VENTILATION","90PZS SOLAR POWER 1370","HOPPECK",24,48,2,1370,{"$nulls":4},52,32,35,"Haut",null,"18:38","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.72,2.7,3.16,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"DEGRADATION",null,null,null,"PAS DE VENTILATION","Bon","CUMMINS","01/01/2016","Non Fonctionnel","01/06/2020",{"$nulls":7},2,null,22,400,50,null,null,12,"75","C 22 D5","MF DIN 75","Manuel","Non",null,"Oui",1,40,1,"Oui","A CAUSE DE LA BATTERIE DEFECTUEUSE",168,null,5.0599999999999996,1,22,"CANADIAN SOLAR","CS 6P - 230P","Mono",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},160,13,"18:04",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},1,null,null,null,9,0,45,835,21,"3*35","4*16","REMPLACER 17 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35 mm2",2,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",{"$nulls":5},"Opérateur",{"$nulls":8},2,{"$nulls":24},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non"]
["P23","1412030101700","14/07/2020","SEDHIOU","SEDHIOU","BAMBALI","MASSARIA",73,1603,2019,"01/01/2015","09/02/2018",0,"NS RESIF","ERSEN II",20,10,5,null,35,"MAMADOU DIAITE SADIO",778390916,"MARAICHAGE","Non","Non",null,null,431576,1389412,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",18.5,null,17.100000000000001,null,1.96,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,22,null,null,null,5.76,2.85,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,"RAFRAICHIR PEINTURE PARTIE EXTERNE",null,"CHANGER SERRURES LOAUX ONDULEUR ET BATTERIE",null,"RAFRAICHIR LA PEINTURE  PARTIE EXTERNE","DEGRADATION DE LA COURONNE DE PROTECTION",2.61,2.4500000000000002,3.15,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":7},"REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,4.5999999999999996,1,5,{"$nulls":11},48,null,750,21.7,56,null,22,null,230,220,240,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.21,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"UNE PARTIE DE LA TOITURE EST EMPORTE PAR LE VENT","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","90PZS SOLAR POWER 1370","HOPPECKE",24,48,2,1370,{"$nulls":4},45,32,null,"Equilibré",null,"16:27","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.75,2.67,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"PAS DE VENTILATION","Mauvais","CUMMINS",null,"Non Fonctionnel",{"$nulls":10},22,400,50,{"$nulls":4},"C22D5",null,"Manuel",{"$nulls":10},5.0599999999999996,1,22,"CANADIAN SOLAR","CS 6P -230 P","Mono",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},19,null,null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"A remplacer",{"$nulls":8},3,2,7,4,50,200,31,"3*35","4*16","REMPLACER 24 PORTEES DE 4X16 mm2 PAR UNE CABLE DE 3X35 mm2",3,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},1,{"$nulls":24},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non"]
["P24","1412030100100","14/07/2020","SEDHIOU","SEDHIOU","BAMBALI","BADIARY",64,2125,2019,"01/01/2013","01/01/2017",0,"NS RESIF","ERSEN II",13,12,10,2,37,"YORO DIEYTE",776174279,null,"Non","Oui",10000,"Oui",438716,1395909,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",22.1,null,21.9,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,3,null,null,4.9800000000000004,5.76,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,null,"LOCAL BATTERIE","REMPLACER SERRURE DES LOCAUX BATTERIE ET ONDULEUR",null,"RAFRAICHIR LA PEINTURE COTE EXTERNE","DEGRADATION DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.7,2.4700000000000002,3.75,"Mauvais Etat","A Remplacer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","A réparer",{"$nulls":7},"REMPLACER LA SERRURE","RAFRAICHIR LA PENTURE",null,"PAS DE VENTILATIN",{"$nulls":36},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.22,2.4700000000000002,3,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,"PRESENCE DE FISSURES","UNE PARTIE DE LA TOITURE EST EMPORTEE PAR LE VENT","REMPLACER SERRURE","LES FENETRES SE DEGRADENT","RAFRAICHIR LA PEINTURE","DEGRADATION DU PLANCHER",null,"PAS DE VENTILATION",{"$nulls":16},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.74,2.75,2.95,"Bon Etat",null,"Mauvais Etat","A réparer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"PRESENCE DE TROUS","DEGRADATION PLANCHER",null,"RAFRAICHIR PEINTURE","RAFRAICHIR PEINTURE","PAS DE VENTILATION",null,"GREEN POWER GP 22","01/01/2013","Non Fonctionnel","01/01/2019",{"$nulls":10},240,50,15,null,null,null,"GP 22 SH/ PW- A",null,"Automatique","Non",null,"Oui",1,40,1,"Oui","BATTERIE DEFECTUEUSE",{"$nulls":37},"Bois","LBC","Bon",null,"Bon",null,"A réparer",{"$nulls":10},9,3,9,9,44.3,445,50,"3*35","4*16","REMPLACER 19 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35 mm2",6,null,6,1,1,"Oui",null,"Oui","Oui","Oui","Conducteur",{"$nulls":5},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,1,1,{"$nulls":11},"Opérateur",null,null,"Opérateur",{"$nulls":5},3,10,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non"]
["P25","1412020202300","13/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","YACINE TAMBANA",50,600,2019,"01/01/2014",0,4,"NS RESIF","ERSEN II",16,9,5,3,33,"MAMADOU FATY",782675938,"MECANICIEN","Non","Oui",10000,"Non",415702,1410533,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",17.8,null,14.74,null,1.67,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",{"$nulls":4},7.4,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"Mauvais état","A réparer",null,"FISSURES ET TROUS","CHANGER SERRURES DES LOCAUX ONDULEUR ET BATTERIE",null,"RAFRAICHIR LA PEINTURE PARTIE EXTERIEURE DU MUR","DEGRADATION DE LA COURONNE DE PROTECTION PERRIPHERIQUE",2.74,2.5,2.95,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":6},"PRESENCE DE FISSURES ET TROUS","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4.5999999999999996,46,306,7,4.2,230,229,{"$nulls":5},48,null,550,21.7,56,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2300000000000004,2.5,3.24,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE DE TROUS ET FISURES","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","10 OPZS 1000","HOPPECKE",22,44,2,1000,null,null,90,null,48,31,32,"Haut",null,"16:48","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.73,2.73,2.95,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":8},12,null,null,240,50,15,null,12,"100","GP 22 SH/ PW- A","6 - QA - 100","Manuel","Non",null,"Oui",1,40,1,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",{"$nulls":5},311,10,"16:06",null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"A remplacer",{"$nulls":6},2,null,2,1,5,2,39.1,78.2,21,"3*35","4*16","17 PORTEES DE 4X16mm2 A REMPLACER PAR UN CABLE DE 3 X 35mm2",7,2,10,6,2,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Opérateur",null,null,1,30,40,20,1,null,null,null,"Opérateur",null,null,"Opérateur",{"$nulls":5},"Opérateur",null,null,null,2,2,null,4,"Non","Non","Non","Non","Non","Non",null,null,2,null,"Non"]
["P26","1412020202400","13/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","YACINE MANDINA",54,677,2019,"01/01/2012",0,2,"NS RESIF","ERSEN II",5,18,3,2,28,"MOUSSA MANE",703069600,"CULTIVATEUR","Non","Oui",10000,"Non",419578,1413376,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.309999999999999,null,17.059999999999999,null,1.74,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,26.4,null,null,null,7.54,5.84,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer",{"$nulls":5},"DEGRADATION DE LA COURONNE DE PROTECTION DU LOCAL TECHNIQUE",2.5,2.75,3.23,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,6,1,4.5999999999999996,{"$nulls":11},48,null,550,26.1,50,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2019",null,2.4900000000000002,4.21,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":8},"PAS DE VENTILATION","10OPZS 1000","HOPPECKE",18,36,2,1000,{"$nulls":5},29,null,"Bas","01/01/2019","11:07","Mauvais Etat","Bon Etat","Mauvais Etat","Mauvais Etat",2.76,2.75,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":6},"PRESENCE DE FISSURES",null,"INFILTRATIONS D'EAU","PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2012","Fonctionnel",{"$nulls":8},12,null,null,240,50,15,null,12,"100","GP 22 SH /PW-A","MF DIN 100","Manuel","Non",null,"Oui",1,40,2,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"A réparer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,"Bon",null,"Mauvais","A remplacer",null,null,null,1,null,16,null,null,"Bois","LBC","Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer","Bon",null,null,null,2,null,null,1,2,0,2,11,0,40.5,340,54,"3*35","4*16","REMPLACER 41 PORTEES DE 4X16mm2 PAR UN CABLE DE 3 X35 mm2",null,null,4,{"$nulls":4},"Oui","Oui",null,"Conducteur",{"$nulls":5},"Conducteur",null,null,"Conducteur",{"$nulls":5},1,null,1,40,{"$nulls":4},"Opérateur",null,null,"Opérateur",{"$nulls":5},"Opérateur",null,null,null,4,30,null,1,"Non","Non","Non","Non","Non","Non",null,null,null,1,"Non",{"$nulls":4},"L'OPERATEUR RCUPERE TOUS LES DECHETS"]
["P27","1412020200600","12/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","DIAFILON DIOLA",53,880,2019,"01/01/2012","01/01/2015",0,"NS RESIF","ERSEN II",7,8,5,null,20,"YOUSSOUF SANE",777931681,"CULTIVATEUR","Non","Oui",10000,"Oui",409116,1411323,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",20.56,null,15,null,1.87,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,4,null,"Autre","RAFRAICHIR PEINTURE PORTES ET POTEAUX",5.75,5.81,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"RAFRAICHIR PEINTURE COTE EXTERNE MUR","PLUSIEURS TROUS","SERRURES A REMPLACER",null,"RAFRAICHIR LA PEINTURE",null,2.54,1.77,3.11,"Mauvais Etat","A Remplacer","A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":4},"QUELQUES DEGRADATIONS",null,null,"SERRURES A CHANGER",null,"A RAFRAICHIR","PAS DE VENTILATION",{"$nulls":6},1,null,1,{"$nulls":27},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.44,2.48,3.16,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"PRESENCE DE TROUS","SERRURE A REMPLACER",null,"A RAFRAICHIR",null,null,"PAS DE VENTILATION","8 OPZS 800","HOPPECKE",24,48,2,800,{"$nulls":4},78,32,null,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.72,1.97,2.87,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"INFILTRATION D'eau . LE PLANCHER COMMENCE A SE DEGRADER",null,null,null,"PAS DE VENTILATION","Bon","CUMMINS",{"$nulls":12},11,400,50,{"$nulls":4},"C11D5",null,"Manuel","Non",{"$nulls":9},5.04,3,12,"ET SOLAR","ET P 636140","Mono",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A réparer",null,null,"Bon",{"$nulls":5},78,16,"13:44",null,"Bois",null,"Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A remplacer",1482,35,27,1,null,1,34,1,null,8,1,57,9100,40,"3*35","4*16",null,4,1,2,null,2,"Oui","Oui","Oui",null,"Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",{"$nulls":5},"Opérateur",null,null,1,1,1,null,1,null,null,null,"Opérateur",{"$nulls":8},"Opérateur",null,null,null,3,null,null,4,"Non","Non","Non","Non","Non","Non",null,2,null,null,"Non"]
["P28","1412020201400","17/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","KOOLING",39,811,2019,"01/01/2014",0,5,"Sud Solar System","ERSEN II",8,8,11,null,27,"ALASSANE SECK MANE",771795243,"CULTIVATEUR","Non","Oui",10000,"Oui",409121,1411326,"Solaire_GE","Oui","Inondable","Non Immatriculé","Oui",19.77,null,17.11,null,1.8,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,4,"Autre","RAFRAICHIR LA PEINTURE",7.52,5.77,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"A réparer",null,"A réparer",null,"PEINTURE PARTIE EXTERNE A RAFRAICHIR","TOITURE LOCAL BATTERIE FISSURE",null,null,null,"COURONNE DE PROTECTION PERIPHERIQUE EN TRES MAUVAIS ETAT",2.67,2.48,3.1,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":6},"PRESENCE DE FISSURES","SERRURES A REMPLACER",null,null,"PAS DE VENTILATION","Onduleur Réseau",null,null,"Monophasé",null,"SUNNY BOY",null,null,1,4.5999999999999996,null,296,{"$nulls":11},550,null,null,20,22,null,null,230,null,null,null,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.22,2.48,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,null,"PRESENCE DE FISSURES","SERRURE A REMPLACER",null,"PEINTURE A RAFRAICHIR","PRESENCE DE TROUS",null,"PAS DE VENTILATION","10OPZS 1000","HOPPECKE",23,46,2,1000,{"$nulls":4},43,28,30,"Bas","01/04/2020","18:59","Mauvais Etat","Mauvais Etat","Bon Etat","Bon Etat",2.74,2.7,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"TOITURE FISSURE",null,"PEINTURE A RAFRAICHIR",null,null,"PAS DE VENTILATION","Bon","GREEN POWER GP22","01/01/2017","Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GP 22 SH / PW_ A",null,"Manuel","Non",null,"Oui",null,30,4,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A réparer","Bon",null,"Mauvais",{"$nulls":5},350,11,"14:05",null,"Bois","LBC","Bon",null,"Mauvais","A remplacer","Bon",null,"Mauvais","A remplacer",null,null,1,null,null,2,null,8,null,8,8,43.3,null,35,"3*35","4*16","REMPLACER 29 PORTEES DE 4X16mm2 PAR UN CABLE DE 3X35mm2",5,null,2,2,3,"Oui",null,"Oui","Oui","Oui","Conducteur",{"$nulls":5},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},30,30,{"$nulls":4},"Opérateur",null,null,"Opérateur",{"$nulls":9},2,2,null,null,"Non","Non","Non","Non","Non","Non",null,null,1,1,"Non"]
["P29","1412020201500","11/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","NEMA DIAOUR",30,500,2019,"01/01/2014",0,12,"NS RESIF","ERSEN II",1,5,8,1,15,"YACOUBA CISSE",775232643,"COURTIER","Non","Non",10000,"Non",405229,1405345,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.2,null,17.600000000000001,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,1,"Autre","RAFRAICHIR PEINTURE",7.5,5.76,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","A réparer",null,null,"PRESENCE DE TROUS","CHANGER SERRURES ONDULEUR ET BATTERIE",null,"RAFRAICHIR PEINTURE EXTERNE DU MUR","PLUSIEURS TROUS AU NIVEAU DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.74,2.5,3.25,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER SERRURE",null,null,"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4.5999999999999996,49,315,null,2.1,229,230,{"$nulls":5},48,125,440,21.7,56,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2019",null,4.21,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":5},"RAFRAICHIR PEINTURE","PRESENCE DE TROUS",null,"PAS DE VENTILATION","10OPZS 1000","HOPPECK",23,46,2,1000,null,null,28,1202,49,30,31,"Equilibré",null,"12:53","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.74,2.74,2.94,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":6},"FISSURES SUR LE MUR","RAFRAICHIR PEINTURE",null,"PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":8},12,null,null,240,50,15,null,12,"75","GP 22SH/ PW- A","DIN 75 MF","Manuel","Non",null,"Oui",null,30,2,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"A réparer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",{"$nulls":5},292,null,"14:17",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",{"$nulls":5},1,null,7,null,null,7,44.4,null,22,"3*35","4*16","COUVERTURE DU RESEAU MAIS TOUTES LES MENAGES NE SONT PAS ABONNES",2,null,3,3,null,"Oui",null,"Oui","Oui",null,"Conducteur",{"$nulls":5},"Conducteur",null,null,"Opérateur",{"$nulls":5},2,{"$nulls":7},"Opérateur",null,null,"Opérateur",{"$nulls":5},"Opérateur",null,null,null,3,2,null,3,"Non","Non","Non","Non","Non","Non",null,null,1,null,"Non",null,null,"Non",null,"UNE BATTERIE LAISSEE DANS LE LOCAL BATTERIE"]
["P30","1412020200400","10/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","DANDONE",42,1000,2019,"01/01/2013",0,4,"NS RESIF","ERSEN II",5,7,10,4,26,"MOUSSA SANE",771511450,"CULTIVATEUR","Non","Oui",15000,"Oui",4007534,1423559,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.8,null,16.899999999999999,null,1.83,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,9,null,null,7.5,5.7,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Mauvais état","A réparer",null,"INFILTRATION D'eau DANS LE LOCAL BATTERIE","CHANGER SERRURE LOCAL ONDULEUR",null,"PEINTURE A RAFRAICHIR","PRESENCE DE QUELQUES TROUS . COURONNE DE PROTECTION A REFECTIONNER",2.8,2.6,3.05,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4.5999999999999996,{"$nulls":11},48,null,550,21.7,56,20,22,null,230,null,230,null,50,50,60,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.3,2.56,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,null,null,"SERRURE A REMPLACER","","A RAFRAICHIR","PRESENCE DE TROUS",null,"PAS DE VENTILATION","10 OPZS 1000","HOPPECKE",19,38,2,1000,{"$nulls":4},33,32,null,null,"01/01/2019","18:21","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.8,2.8,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"PEINTURE A RAFRAICHIR",null,null,"PAS DE VENTILATION","Bon","GREEN POWER GP22","01/01/2014","Fonctionnel",{"$nulls":4},245,null,null,null,12,null,null,240,50,15,null,12,"100","GP22 SH / PW - A","MF DIN 100","Manuel","Non",null,"Oui",1,30,4,"Non",null,null,"01/01/2019",5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A réparer","Bon",null,"Bon",{"$nulls":5},347,6,"19:06",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais","A remplacer",{"$nulls":5},1,null,10,1,0,10,49.9,1100,35,"3*35","4*16","22 PORTEES DE 16mm2 A REMPLACER PAR UN CABLE DE 3X35mm2",2,1,2,1,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":5},3,1,1,30,{"$nulls":7},"Opérateur",{"$nulls":5},"Opérateur",{"$nulls":4},30,null,30,"Non","Non","Non","Non","Oui","Non",{"$nulls":9},"LES 10 BATTERIES DEFECTUEUSES SONT ABANDONNES DANS LE LOCAL BATTERIE"]
["P31","1412020201100","10/07/2020","SEDHIOU","SEDHIOU","SANSAMBA","KAMOYA",44,1000,2019,"01/01/2011","01/02/2020",0,"NS RESIF","ERSEN II",4,10,5,4,23,"BOUBACAR DIEDHIOU",771598456,"PAYSAN","Non","Oui",10000,"Oui",405657,1422215,"Solaire_GE","Non","Inondable","Non Immatriculé","Oui",18,null,17,null,1.5,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",10,2,null,null,7.5,6,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Mauvais état","A réparer",null,"FISSURES","REMPLACER SERRURE LOCAL ONDULEUR",null,"RAFRAICHIR PEINTURE LOCAL TECHNIQUE","PRESENCE DE TROUS AU NIVEAU DE LA COURONNE DE PROTECTION PERIPHERIQUE",2.4500000000000002,2.7,2.9,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":4},"PRESENCE DE TROUS",null,"FISSURE","REMPLACER SERRURE",null,"RAFRAICHIR PEINTURE","PAS DE VENTILATION","Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND","SUNNY BOY",1,5,1,4.5999999999999996,null,381,{"$nulls":9},48,440,550,21.7,56,20,22,null,230,null,230,null,50,50,60,"Fonctionnel","A remplacer","Fonctionnel",null,"Non",null,"01/01/2019",null,4.3,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,null,"FISSURES",null,null,"RAFRAICHIR PEINTURE",null,null,"PAS DE VENTILATION","10 OPZ S 1000","HOPPECKE",20,40,2,1000,{"$nulls":4},35,32,32,"Bas",null,"13:29","Bon Etat","Bon Etat","Mauvais Etat","Mauvais Etat",2.95,2.7,2.68,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":4},"FISSURES",null,"PEINTURE A RAFRAICHIR",null,null,"PAS DE VENTILATION","Bon","GREEN POWER GP 22","01/01/2011","Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GP 22 SH / PW- A","BATTERIE ENLEVEE","Manuel","Non",null,"Oui",1,60,3,"Non",null,null,null,5.16,1,24,"REC SOLAR","REC 215 AE","Mono",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",null,2,null,null,null,377,16,"13:55",null,"Bois","LBC","Bon",null,"Bon",null,"A remplacer","A réparer","Mauvais","A remplacer",{"$nulls":5},5,3,2,2,10,2,23.1,1300,47,"3*35","4*16","20 PORTEES DE 4X16mm2 A REMPLACER PAR UN CABLE DE 3 X35mm2",4,null,4,null,null,"Oui",null,"Oui",null,null,"Conducteur",{"$nulls":5},"Conducteur",{"$nulls":8},2,null,1,{"$nulls":5},"Opérateur",null,null,"Opérateur",{"$nulls":9},2,null,null,null,"Non","Non","Non","Non","Non","Non",2,1,4,null,"Non",{"$nulls":4},"4BATTERIES DEFECTUEUSES ET UN LAMPADAIRE LAISSES DANS LE LOCAL BATTERIE"]
["P32","1432010201400","14/07/2020","SEDHIOU","GOUDOMP","KAOUR","SINGHERE BAYNOUCK",53,1152,2020,"01/01/2014","01/09/2019",0,"Sud Solar System","ERSEN II",6,14,11,5,36,"ABDOULAYE BIAYE",776308817,"3é secondaire","Non","Non",10000,"Oui",397776,1386025,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,72,null,"Serrure",null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état","A réparer",null,"14 ARDOISES FIBRO CIMENT",null,null,"A REPRENDRE","A REPARER",2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat","A Remplacer",{"$nulls":5},"6 ARDOISES FIBRO CIMENT A REMPLACER",{"$nulls":4},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","5048","5000 TL -20",1,5,1,5,{"$nulls":10},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"A REPRENDRE",null,null,null,"90 PZS 1370 AH + ROLLS","HOPPECKE + ROLLS",null,39,2,1370,{"$nulls":4},39.4,null,null,"Bas","01/12/2019","14:50","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.7,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"8 ARDOISES FIBRO CIMENT",{"$nulls":5},"Bon","GREEN POWER GP 22","01/01/2014","Non Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GP 22 SH/ PW- N A",null,"Manuel","Non",null,"Non",null,null,null,"Non",null,null,null,5.0599999999999996,2,11,"CANADIAN SOLAR","CS 6 P - 230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":6},13,"17:15",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":12},40,null,null,"4*16",null,null,4,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},7,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,4,{"$nulls":4},"Non","Non","Non","Non","Non","Non",null,null,4,null,"Non",null,null,"Non"]
["P33","1432030100200","14/07/2020","SEDHIOU","GOUDOMP","NIAGHA","BAMBADALA 1",56,900,2020,"01/01/2012",0,5,"Faye Solaire_Sud Energie","ERSEN I",19,13,3,1,26,"SAMBA MANDIANG",776789522,"PAS DE NIVEAU","Non","Non",20000,"Oui",466321,1402863,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,null,"Serrure",null,7.5,5.7,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,null,"1 SERRURE",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":6},"1 SERRURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 R 20",1,5,1,5,48.6,null,null,null,229.9,null,51.81,null,null,null,41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,"01/01/2018",null,4.2,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"1 SERRURE",null,"A REPRENDRE",null,null,null,"10 CPZS 1000 AH","HOPECKE",22,48,2,1000,null,null,86,null,48.4,null,30.1,"Bas",null,"16:24","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":8},"Bon","GREEN POWER GP","01/01/2012",{"$nulls":12},240,50,15,null,null,null,"GP 22 SH /PW-N-A",null,"Manuel","Non",null,"Non",null,null,null,"Non",null,null,null,4945,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.6,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":7},"Bon",null,1,{"$nulls":4},14,null,null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},6,6,35,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",1,null,2,null,"Non",null,null,"Non"]
["P34","1432030101100","14/07/2020","SEDHIOU","GOUDOMP","NIAGHA","KITIM",66,1300,2020,"01/01/2012","01/12/2019",0,"Sud Solar System","ERSEN II",5,null,1,4,10,"YAYA BALDE",772600651,"5é SECONDAIRE","Non","Non",10000,"Oui",462758,1401498,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",306,28,"Serrure",null,7.5,5,"Oui","Bon état",null,"Mauvais état","A réparer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"2 ARDOISES","2 SERRURES",null,"A REPRENDRE",null,2.7,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":6},"1 SERRURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048 SMA","SB 5000 TL - 20 SMA",1,5,1,5,{"$nulls":10},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",2,"01/01/2019",null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"2 ARDOISES","1 SERRURE",null,"A REPRENDRE",null,null,null,"10 OPZS 1000","HOPPECKE",21,39,2,1000,{"$nulls":7},"Equilibré",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GP 22",{"$nulls":13},240,50,15,null,null,null,"GREEN POWER GP 22 SH/PW-N-A",null,"Manuel","Non",{"$nulls":5},"Non",null,null,null,5160,2,12,"REC","REC 215 AE","Poly",215,7.6,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":7},"Bon",null,1,{"$nulls":4},11,null,"08/08/2020","Bois",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},8,8,35,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P35","1432030400800","15/07/2020","SEDHIOU","GOUDOMP","DIOUBOUDOU","SANOUFILY",55,1035,2020,"01/01/2014",0,2,"Faye Solaire_Sud Energie","ERSEN II",22,19,2,6,49,"ABDOUL AZIZ SAGNA",783392791,"6é SECONDAIRE","Non","Non",10000,"Oui",445503,1399258,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",19,19,17,17,1.7,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Bon Etat",null,72,null,"Serrure",null,7.5,5,"Non","Bon état",null,"Mauvais état","A remplacer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"30 ARDOISES FIBRO CIMENT","2 SERRURES",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A Remplacer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"8 FIBRO CIMENT","1 SERRURE",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL 20",1,5,1,5,{"$nulls":10},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 ARDOISE","1 SERRURE",null,"A REPRENDRE",null,null,null,"90PZS 1370 AH","HOPPECKER",24,51,2,1370,{"$nulls":7},"Bas",null,"14:20","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.7,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"8 ARDOISES",{"$nulls":5},"Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":11},240,50,15,null,12,"75","GREEN POWER GP 22","ENERGY","Manuel",null,null,"Oui",1,20,null,"Non",null,null,null,5060,2,11,"CANADIAN","CS6P-230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":9},"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},8,8,40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},3,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,2,{"$nulls":4},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P36","1432030400600","16/07/2020","SEDHIOU","GOUDOMP","DIOUBOUDOU","MALANDIANKUNDA",45,1300,2020,"01/01/2015",0,2,"Faye Solaire_Sud Energie","ERSEN II",16,12,7,3,38,"YAYA FATY",779717599,"ARABISAN","Non","Non",15000,"Oui",444007,1402374,"Solaire_GE","oui","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",70,2,"Serrure",null,7.5,5.5,"Non","Bon état",null,"Mauvais état","A remplacer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"30 ARDOISE FIBRO CIMENT","1 SERRURE",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A Remplacer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":4},"8 ARDOISES FIBRO CIMENT","1 SERRURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL -21",1,5,1,5,51.5,293,4.45,3.1,229.9,231,49.9,null,null,null,41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"10 ARDOISES",null,null,"A REPRENDRE",null,null,null,"90PZS 1370 AH","HOPPECKE",22,50,{"$nulls":4},90.9,2.2000000000000002,50.8,32,31.7,"Equilibré",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.6,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,null,"8 ARDOISES FIBRO CIMENT",null,null,"CADENAS",null,null,"Bon","GREEN POWER GP22","01/01/2015","Fonctionnel",{"$nulls":11},240,50,15,null,12,"100","GP 22 SH/PW - N-A","MF DIN 100","Manuel","Non",null,"Oui",3,120,null,"Non",null,null,null,4830,2,11,"CANADIAN SOLAR","CS6P - 230","Poly",230,7.78,29.6,38.799999999999997,8.34,"Mauvais",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":6},20,"14:54",null,"Bois",null,"Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":9},1,6,1,40,null,null,"4*16",null,null,4,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,2,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P37","1432010402400","16/07/2020","SEDHIOU","GOUDOMP","SIMBADI BALANTE","SAFANE",115,986,2020,"01/01/2015","01/01/2020",0,"Faye Solaire_Sud Energie","ERSEN II",23,12,3,3,41,"IBRAHIMA DIATTA",782341906,"1é SECONDAIRE","Non","Non",10000,"Oui",421885,1381885,"Solaire_GE","Non","Non Inondable","Délibération","Oui",23,23,18,18,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},8,6,"Oui","Bon état",null,"Mauvais état","A remplacer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"30 ARDOISES",null,null,"A REPRENDRE",null,3.2,3,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"8 ARDOISES",null,null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 500 TL -20 et sb 2500",2,5,2,5,{"$nulls":10},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,3,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"10 ardoises",null,null,"a reprendre",null,null,null,"9 ORZS 1370 AH","HOPPECKE",23,37,2,1370,{"$nulls":4},37.9,null,null,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",3.2,3.2,2.6,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"8 ARDOISES",{"$nulls":5},"Bon","GREEN POWER GP 22","01/01/2015","Fonctionnel",{"$nulls":11},400,50,20,null,12,"100","POLAR TAB","S 10H 60044 SMF","Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,7590,3,11,"CANADIAN","CS6P - 230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",{"$nulls":16},23,"11:20",null,"Bois",null,"Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":7},1,null,null,13,13,35,null,null,"4*16",null,null,12,{"$nulls":4},"Oui","Non","Non","Non","Non","Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":8},"Non","Non","Non","Non","Non",null,2,1,null,"Non",null,null,"Non"]
["P38","1432030300700","13/07/2020","SEDHIOU","GOUDOMP","BAGHERE","FRANCOUNDA",34,586,2020,"01/01/2014","01/02/2020",0,"Sud Solar System","ERSEN II",9,8,12,4,33,"SOUNKAR DANFA",779475474,"CM2","Non","Non",20000,"Oui",457980,1393887,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,16,16,1.7,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,null,null,"Serrure",null,7.5,5,"Non","Bon état",null,"Mauvais état","A réparer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"2 ARDOISES A CHANGER","2 SERRURES A CHANGER",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A réparer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"1 ARDOISE FIBRO CIMENT A CHANGER","1 SERURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048 SMA","SB 5000TL 20 SMA",1,5,1,5,{"$nulls":10},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 FIBRE CIMENT","1 SERRURE",null,"A REPRENDRE",null,null,null,"9OPZS SOLAR POWER","HOPPECKE",22,28,2,1370,null,null,null,1.85,null,null,32,"Bas",null,"17:18","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GP 22","01/01/2014","Non Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GREEN POWER GP 22 SH /PW -N-A",null,"Manuel","Non",null,"Oui",1,20,null,"Non",null,null,null,5060,2,11,"CANDIAN SOLAR","CS6P 230 P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":5},279,5,"17:23",null,null,null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},12,12,40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",6,null,2,null,"Non",null,null,"Non"]
["P39","1432030301200","13/07/2020","SEDHIOU","GOUDOMP","BAGHERE","LAMEL",52,1100,2020,"01/01/2012","01/03/2020",0,"Sud Solar System","ERSEN II",12,6,16,4,38,"AMADOU KANDE",766048815,"CM2","Non","Non",10000,"Oui",459169,1393280,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,2.7,null,"Oui","Grillage","Bois","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",null,28,"Serrure",null,7.5,5.5,"Non","Bon état",null,"Mauvais état","A réparer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"1 FIBRO CIMENT","2 SERRURES",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":6},"1 SERRURE","","A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8 AH 12","SB 5000TL 20",1,5,1,5,{"$nulls":10},41,63,175,400,26,120,15,30,230,253,220,240,45,70,45,55,"Non Fonctionnel",null,"Fonctionnel",null,"Oui",2,"01/01/2018",null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 FIBRO CIMENT","1 SERRURE",null,"A REPRENDRE",null,null,null,"10 OPZS 1000 AH",null,22,42,2,1000,null,null,null,1.95,null,null,30,"Bas",null,"15:57","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":8},"Bon","GREEN POWER","01/01/2012","Non Fonctionnel",{"$nulls":11},240,50,15,null,12,"102","GREEN POWER GP","TROSAN","Manuel","Non",null,"Oui",1,20,null,"Non","BATTERIE DEFAILLANTE",null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.6,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":5},348,20,null,null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},6,6,40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},2,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":8},"Non","Non","Non","Non","Non",null,1,2,null,"Non",null,null,"Non"]
["P40","1432030300601","13/07/2020","SEDHIOU","GOUDOMP","BAGHERE","FADIOUNGHAR",47,804,2020,"01/01/2012","01/02/2020",0,"Sud Solar System","ERSEN II",12,2,4,4,22,"KARIM KANDE",771997490,"PAS DE NIVEAU","Non","Non",20000,"Oui",458071,1392057,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Non","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",73,24,null,null,7.5,5.5,"Non","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"1 FIBRO CIMENT","",null,"A REPRENDRE",null,2.75,2.5,2.9,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",null,null,"FAIRE UNE OUVERTURE",{"$nulls":5},"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 80 OH -12","SB 5000TL 20 SMA",1,5,1,5,{"$nulls":10},41,63,175,400,26,120,15,30,230,253,220,240,45,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 ARDOISE",null,null,"A REPRENDRE",null,null,null,"10 OPZS 1000 AH","HOPPECKE",24,34,2,1000,{"$nulls":7},"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GP 22","01/01/2012",{"$nulls":12},240,50,15,null,12,"100","GREEN POWER GP 22","CROWN","Manuel","Non",null,"Oui",1,20,null,"Non",null,null,null,5.16,2,12,"CANADIAN SOLAR","CS 6P -230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",{"$nulls":9},"Bon",{"$nulls":6},13,"17:45",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":12},40,null,null,"4*16",null,null,10,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},7,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,3,{"$nulls":4},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P41","1432010503300","15/07/2020","SEDHIOU","GOUDOMP","YARANG BALANTE","SINA",53,1047,2020,"01/01/2015","01/07/2019",0,"Faye Solaire_Sud Energie","ERSEN II",9,21,6,4,40,"SECKOU SADIO",779085972,"1é SECONDAIRE","Non","Non",10000,null,484038,1436568,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,20,null,null,null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A remplacer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"30 ARDOISES","2 SERRURES",null,"A REPRENDRE",null,2.95,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A Remplacer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"8 ARDOISES","1 SERRURE",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL 20",1,5,1,5,null,265,2.38,7,229.9,{"$nulls":5},41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,"01/01/2018",null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"10 ARDOISES","1 SERRURE",null,"A REPRENDRE","A REPRENDRE",null,null,"9 OPZS SOLAR POWER 1370 AH","HOPPECKE",24,42,2,1370,null,null,93.8,1.75,42,32,39.700000000000003,"Equilibré",null,"14:13","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.6,2.7,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":4},"8 ARDOISES",null,null,"A REMPLACER",null,null,"Bon","GREEN POWER GP 22",null,"Non Fonctionnel",{"$nulls":11},240,50,15,null,12,"100","GP 22 SH/PW -N-A","TAB POLAR","Manuel","Non",null,"Oui",1,20,2,"Non",null,null,null,5060,2,11,"CANADIAN SOLAR","S6P - 230p","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":5},265,20,null,null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"Mauvais",{"$nulls":9},1,9,9,40,null,null,"4*16",null,null,12,{"$nulls":4},"Oui","Non","Non","Non","Non","Conducteur",{"$nulls":14},24,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",null,null,1,null,"Non",null,null,"Non"]
["P42","1432010301200","15/07/2020","SEDHIOU","GOUDOMP","Mangarounkou","KOGNARA",82,2365,2020,"01/01/2014",0,2,"Sud Solar System","ERSEN II",25,6,6,4,41,"IBRAHIMA MANE",779338236,"TERMINALE","Non","Non",20000,"Oui",437227,1387715,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,1.8,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"Serrure",null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Mauvais état","A réparer",null,"30 ARDOISES","2 SERRURES",null,"A REPRENDRE","A REPARER",2.8,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer",null,null,null,"A REPARER",null,"8 ARDOISES","1 SERRURE",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL 20",1,5,1,5,59.7,258,6.2,7.6,229.9,234,49.99,null,null,null,41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,null,"10 ARDOISES","1 SERRURE",null,"A REPRENDRE","A REPARER",null,null,"9OPZS 1370 AH","HOPPECKER",24,53,2,1370,null,null,67.400000000000006,null,53.8,null,71.3,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.8,2.75,2.7,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":4},"8 ARDOISES",null,null,"CHAINE + CADENAS",null,null,"Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":11},240,50,25,null,12,"75","GREEN POWER GP 22","POKYOU LIGHT BIN 75 MF","Manuel","Non",null,"Oui",1,20,1,"Non",null,null,null,5060,2,11,"CANADIAN SOLAR","CS 6P -230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":5},258,16,null,null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":12},40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,2,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,7,null,null,null,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P43","1432010301900","15/07/2020","SEDHIOU","GOUDOMP","Mangarounkou","SEGAFOULA",68,1413,2020,"01/01/2014","01/05/2020",0,"Sud Solar System","ERSEN II",25,6,9,5,45,"MALANG SANO",771910728,"ARABE","Non","Non",20000,"Oui",439407,1389455,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,2.9,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,70,null,null,null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","A remplacer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"4 ARDOISES A REMPLACER","2 SERRURES",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":6},"1 SERRURE",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL -20",1,5,1,5,null,276,2.59,1.8,229.9,231,51.9,null,null,null,41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.25,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"4 ARDOISES","1 SERRURE",null,"A REPRENDRE",null,null,null,"9 OPZS 1370 AH","HOPPECKE",21,48,2,1370,null,null,80.3,null,48.3,null,34.1,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.75,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",{"$nulls":5},"CHAINE + CADENAS",null,null,"Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":11},240,50,15,null,12,"75","GD 22 SH/PW - N-A","TNT 12V 75 AH DIN 75","Manuel","Non",null,"Oui",1,20,2,"Non",null,null,null,5060,2,11,"CANADIAN","CS6P 230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Mauvais",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":5},276,13,"11:45",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",{"$nulls":14},40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui","Non","Non","Non","Non","Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,24,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":8},"Non","Non","Non","Non","Non",2,null,5,null,"Non",null,null,"Non"]
["P44","1012010203300","17/07/2020","KOLDA","KOLDA","MEDINA  EL HADJI","SARE KOUBE",67,1030,2020,"01/01/2007",0,10,"Sud Solar System","ERSEN I",23,5,null,1,29,"ABDOULAYE KANDE",771595141,"PAS DE NIVEAU","Non","Non",10000,"Oui",514606,1402099,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",20,20,15,18,1.8,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Bon Etat",null,76,null,null,null,6,5.9,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",{"$nulls":5},"A REPRENDRE",null,2.5,2,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":8},"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé",null,"STECA STUDER",null,1,6,null,null,48.8,null,20,null,null,null,50,null,null,null,38,68,null,null,null,70,null,null,230,265,null,null,45,65,null,null,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,3.3,2.5,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"A REPRENDRE",null,null,null,"9 OPZS 1370 AH","HOPPECKE",23,49,2,1370,null,null,19,null,48.5,null,null,"Equilibré","09/08/2020",null,"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.75,2,2.4,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","CUMMINS","01/01/2007","Fonctionnel",{"$nulls":11},240,50,11,null,null,null,"CUMMINS GP",null,"Manuel","Non",{"$nulls":5},"Non",null,null,null,5100,3,10,"SCHOTT SOLAR","D- 63755","Poly",170,4.71,44,36,5.25,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",{"$nulls":5},"Bon",null,5,{"$nulls":4},17,"10:23",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},4,4,35,null,null,"4*16",{"$nulls":12},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,2,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,{"$nulls":4},"Non","Non","Non","Non","Non","Non",null,1,null,2,null,null,null,"Non"]
["P45","1012030200200","17/07/2020","KOLDA","KOLDA","THIETTY","DIASSINA",63,375,2020,"01/01/2007","01/01/2010",0,"Sud Solar System","ERSEN I",3,8,2,4,17,"AMADOU SEYDI",783867872,"PAS DE NIVEAU","Non","Non",10000,"Oui",484038,1436568,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,20,18,18,1.5,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",76,28,null,null,6,6,"Oui","Bon état",null,"Mauvais état","A remplacer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"5 ARDOISES A CHANGER","A CHANGER",null,"A REPRENDRE",null,2.5,1.9,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":8},"A REPRENDRE",null,"Onduleur Réseau",{"$nulls":5},1,6,{"$nulls":12},38,68,null,null,null,70,null,null,230,265,null,null,45,65,null,null,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,3.4,2.5,2.8,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"3 ARDOISES",null,null,"A REPRENDRE",null,null,null,"OPZS 800 AH","HOPPECKE",16,null,2,800,{"$nulls":7},"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.75,1.95,2.44,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"2 ARDOISES FIBRO CIMENTS",{"$nulls":5},"Bon","CUMMINS GP","01/01/2007","Non Fonctionnel","01/01/2010",{"$nulls":10},240,50,11,null,null,null,"CUMMINS GP",null,"Manuel","Non",null,"Non",null,null,null,"Non",null,null,null,5.0999999999999996,3,10,"SCHOTT SOLAR","D63755","Poly",170,4.71,44,36,5.25,"Bon",null,"Bon",null,"A remplacer",null,"Mauvais",null,"A réparer",{"$nulls":5},"Bon",null,3,{"$nulls":7},"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},6,6,45,null,null,"4*16",null,null,8,{"$nulls":4},"Oui","Non","Non","Non","Non","Conducteur",{"$nulls":19},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",3,null,16,null,null,"2",null,"Non"]
["P46","0922010503300","10/07/2020","FATICK","FOUNDIOUGNE","NIASSENE","NIASSENE",82,1023,2020,"01/04/2016","01/01/2017",0,"SALENSOL","ERSEN II",5,7,6,6,24,"DJIM NIASSENE",775658628,"ECOLE CORANIQUE","Non","Non",5000,"Non",366832,1542723,"Solaire_GE","Non","Inondable","Non Immatriculé","Oui",18,18,18,18,1.5,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",72,26,null,null,7,6,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"1 FEUILLE",{"$nulls":4},2.5,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":47},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 FEUILLE",{"$nulls":6},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,1.18,1.22,46.5,29,29,"Bas",null,"10:21","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.8,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER G22",null,"Non Fonctionnel","04/09/2016",{"$nulls":9},22,400,50,20,null,12,"72","GP 22","57220 MF","Manuel","Non",null,"Oui",1,20,1,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,null,null,"Bon",{"$nulls":5},370,480,null,null,"Bois","Incandescente","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais",{"$nulls":9},3,6,2,35,null,24,null,null,"1 POTEAU SIMPLE 1 JUMELE ET 1 CONTRE FICHE A REMPLACER",1,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,2,30,1,30,30,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,1,1,1,1,"Non","Non","Non","Non","Non","Non",1,2,24,null,"Non",null,null,"Non"]
["P47","0922010503400","10/07/2020","FATICK","FOUNDIOUGNE","NIASSENE","THIAMENE DIOGO",68,586,2019,"01/03/2016","01/01/2017",0,"SALENSOL","ERSEN II",6,null,null,null,68,"BABACAR THIAM",773055030,"MECANICIEN","Non","Non",null,null,365292,1535580,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",18,18,17,17,3,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":5},7.5,5.5,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.75,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",{"$nulls":39},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,null,1.21,44.5,230,31,"Bas",null,"12:47","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,2.6,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",{"$nulls":6},"SERURE",null,null,"Bon","GREEN POWER GP","01/03/2016","Non Fonctionnel","01/01/2017",{"$nulls":9},22,400,50,20,null,12,"66","GP 22","DIN 66MF","Manuel","Non",null,"Oui",1,10,null,"Oui","INJECTEUR",null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,null,null,"Bon",null,2,null,null,null,344,517,"12:57",null,"Bois","Incandescente","Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":7},2,null,2,6,3,45,180,19,"3*35","4*16",null,1,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,10,30,1,20,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",{"$nulls":4},7,null,null,"Non","Non","Non","Non","Non",2,2,24,null,"Non",null,null,"Non"]
["P48","0922010503500","10/07/2020","FATICK","FOUNDIOUGNE","NIASSENE","THIAMENE KEUR SOULEYMANE",34,500,2020,"01/01/2006",0,3,"SALENSOL","ERSEN II",8,10,5,6,31,"EL HADJ THIAM",772700781,"COMMERCE","Oui","Oui",null,"Non",365219,1539257,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.5,18.5,18,18,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Bon Etat",null,null,null,"Autre","GRILLAGE",6.6,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,"6 FEUILLES","SERRURE",null,null,null,2.65,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":6},"1 FEUILLE","SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA S18 OH-12","SMA SB 5000 TL - 20",1,6,1,5,47,321,8.6,8.6,230,231,50,50,null,null,41,63,125,550,null,26,null,22,202,253,180,280,40,70,49.5,50.5,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,"22/01/2020",null,4.5,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"2 FEUILLES","SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,null,1.22,47,33.299999999999997,34,"Bas",null,"15:30","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.8,2.7,2.7,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"3 FEUILLES",{"$nulls":5},"Bon","GREEN POWER","01/05/2016","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"72","GP 22","57220 MF","Manuel","Non",null,"Oui",1,30,2,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},380,493,"16:00",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais","A réparer",{"$nulls":8},2,2,7,45,60,22,"3*70","3*35","22 POTEAUX DONT 1 JUMELE ET 3 CONTRE FICHE",2,10,3,3,null,"Oui","Oui",null,"Non","Non","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,30,30,2,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Conducteur",null,null,null,3,null,1,null,"Non","Non","Non","Non","Non","Non",1,null,24,null,"Non",null,null,"Non"]
["P49","0922010500800","10/07/2020","FATICK","FOUNDIOUGNE","NIASSENE","DIAGANE SADER",57,850,2020,"06/08/2015",0,3,"SALENSOL","ERSEN II",8,17,7,15,37,"BIRANE NDIAYE",776198762,"ELECTRICIEN","Oui","Non",null,"Non",362029,1539900,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18.5,null,16.5,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Bon Etat",null,null,null,"pomelle",null,7.6,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.7,2.4500000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 1700",3,1.5,3,5,47,207,1.1000000000000001,1.3,227,227,50,50,null,null,41,63,139,400,null,120,null,8.6,172.5,264.5,180,260,40,70,45.5,54.5,"Fonctionnel",null,"Fonctionnel",null,"Non",null,"01/01/2018",null,4.2,2.4500000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"10 OPZS 1000","HOPPECKE",24,46,20,1000,55,20,86,1.22,49,32,36,"Bas",null,"17:32","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER","01/08/2015","Fonctionnel",{"$nulls":10},22,400,50,20,null,null,null,"GP 22",null,"Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",null,null,2,null,null,1,220,241,"18:02",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais","A réparer",{"$nulls":7},6,2,4,6,null,null,38,"3*70","3*35","3 CONTRE FICHE  1NJUMELE",4,6,6,4,6,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,2,10,30,30,5,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,2,1,6,7,null,"Non","Non","Non","Non","Non","Non",2,null,24,null,"Non",null,null,"Non"]
["P50","0732010106000","14/07/2020","THIES","TIVAOUANE","MEOUANE","NDOMBIL",80,1190,2016,"08/02/2015",0,4,"ENERSA","ERSEN II",31,36,2,0,86,"ABDOULAYE NIANG",775680266,"ELECTRICIEN","Oui","Oui",null,"Oui",316093,1680165,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",24,40,16,40,1.5,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,null,null,7.3,5.7,"Oui","Bon état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,2.5,2.2000000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000 TL - 20",6,5,2,5,47.52,262,18.600000000000001,18.600000000000001,232,232,{"$nulls":4},41,63,125,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",3,null,null,4,2.2000000000000002,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"OPZS 1000","HOPPECKE",48,48,2,1000,55,20,29,null,52,30.1,33.299999999999997,"Equilibré",null,"12:32","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.5,2.5,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","CUMMINS","01/01/2017","Fonctionnel",null,579.9,33,50,400,481,32,32,12.6,null,33,400,50,30,null,12,"100","C 33D5","MF DIN 100","Manuel","Non",null,"Oui",112016,200,2,"Non",null,null,null,10,4,10,"SUN TECH","STP 250 - 20/ W","Poly",250,8.15,30.7,37.4,8.6300000000000008,"Bon",null,"Mauvais","A réparer","Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,1,null,null,2,279,482,"12:53",null,"Bétons","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer",{"$nulls":6},2,3,4,0,13,40,820,53,"3*70","3*35",null,3,3,1,3,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,45,1,45,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,30,2,1,1,null,"Non","Non","Non","Non","Non","Non",1,null,24,null,"Non",null,null,"Non"]
["P51","0732010107300","14/07/2020","THIES","TIVAOUANE","MEOUANE","SINE MOUSSE ABDOU",98,1412,2020,"01/09/2009","2020-05-01",0,"ENERSA","ERSEN I",30,12,null,null,42,"MODOU SAMB",778005054,"AGRICULTEUR","Oui","Oui",null,"Oui",312501,1679234,"Solaire_GE_Eolienne","Non","Non Inondable","Non Immatriculé","Oui",24,30,16,30,1.5,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,10,null,null,10,5,"Oui","Bon état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,4.5,1.8,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":6},"SERRURE",{"$nulls":4},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA  SI 5048","SMA SB 1700",3,5,3,1.5,58,210,2.1,2.1,228,228,{"$nulls":4},41,63,139,400,null,120,null,8.6,172.5,264.5,180,260,40,70,45.5,54.5,"Non Fonctionnel","A remplacer","Fonctionnel",null,"Oui",8,null,null,4,3.2,2.8,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"12 OPZS SOLAR POWER 2170","HOPPECKE",24,48,2,2170,55,20,90,null,58,29.3,31.5,"Equilibré","01/12/2015","15:50","Bon Etat","Bon Etat","Bon Etat","Bon Etat",4,2.2000000000000002,3.3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":44},10.36,4,12,"REC ET SUNTECH","RE 215 AE  STP 250-20","Poly",250,8.15,30.7,37.4,8.6300000000000008,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,3,null,null,null,245,211,"16:00",null,"Bois","LBC","Bon",null,"Mauvais","A remplacer","Mauvais","A remplacer","Mauvais","A remplacer",null,null,5,null,null,2,5,4,6,0,10,42,820,38,"3*35","4*16",null,5,2,2,null,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,20,1,1,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,2,1,1,15,"Non","Non","Non","Non","Non","Non",3,1,24,null,"Non",null,null,"Non"]
["P52","0922030300700","11/07/2020","FATICK","FOUNDIOUGNE","NIORO ALASSANE TALL","KEUR AMATH SEUNE",70,600,2020,"01/02/2015",0,11,"SALENSOL","ERSEN II",12,7,2,7,28,"ABDOULAYE NIANG",770281448,"BAC ARABE","Oui","Non",null,"Non",362485,1533562,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,null,null,7.5,6.8,"Oui","Bon état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,2.71,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SM SB 5000 TL - 20",1,5,1,5,49.9,328,null,4.4000000000000004,230,230,50,50,null,null,41,63,175,550,null,120,null,622,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.25,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,211,1000,55,20,55,1.23,49.9,28,30,"Bas",null,"11:15","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.71,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"GREEN POWER","01/02/2015","Fonctionnel",{"$nulls":8},12.9,null,22,400,50,20,null,12,"80","GP 22","MF DIN 80","Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":4},1,332,187,"11:35",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A réparer",{"$nulls":8},2,8,1,43,800,30,"3*70","3*35","1 POTEAU JUMELE ET 1 POTEAU SIMPLE SONT A REMPLACER",1,10,2,61,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,5,30,40,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},1,null,null,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P53","0922030103500","11/07/2020","FATICK","FOUNDIOUGNE","KEUR S.DIANE","DRAME IBRA",52,528,2020,"01/02/2016","01/06/2020",0,"SALENSOL","ERSEN II",6,12,6,4,28,"MOKHTAR DIOP",773580820,"CULTIVATEUR","Oui","Non",null,"Non",363845,1530008,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,50.5,18,50.5,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,"Serrure",null,7.75,6.5,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"5 FEUILLES","SERRURE",null,"LOCAL BATTERIE ET GE",null,2.85,2.5,2.68,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":5},"3 FEUILLES","SERRURE",null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000 TL - 20",1,5,1,5,{"$nulls":10},41,63,175,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Non Fonctionnel","A remplacer","Fonctionnel",null,"Oui",4,null,null,4.25,2.58,2.68,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"3 FEUILLES",null,null,"COTE EST",null,null,null,"10 OPZS 1000","HOPPECKE",24,48,20,1000,55,20,null,null,45.8,38,33.200000000000003,"Equilibré",null,"13:30","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.8,2.7,2.5,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,"3 FEUILLES",null,null,"SERRURE",null,null,"Bon","GREEN POWER","01/02/2016","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,null,"GP 22",null,"Manuel","Non",null,"Oui",1,40,3,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":4},1,375,352,"13:40",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A réparer",{"$nulls":6},4,null,2,2,8,45,412,24,"3*35","4*16",null,8,8,8,8,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,30,30,30,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,{"$nulls":4},"Non","Non","Non","Non","Non","Non",null,1,null,null,"Non",null,null,"Non"]
["P54","0922030102000","12/07/2020","FATICK","FOUNDIOUGNE","KEUR S.DIANE","KEUR MOUDIAYE FATIM",48,987,2020,"01/04/2012",0,4,"SALENSOL","ERSEN II",26,4,4,4,38,"MANSOUR SARR",770648887,"ELECTRICIEN","Oui","Non",null,"Non",363449,1521343,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18,null,17,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Bon Etat",{"$nulls":5},7.5,6.7,"Oui","Bon état",null,"Bon état",null,"Mauvais état",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,2.7,2.4500000000000002,2.95,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000 TL - 20",1,5,1,5,48.5,321,4.7,4.7,230,230,50,50,null,null,41,63,175,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.45,2.4500000000000002,2.95,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,14,1.22,48.5,29,31.2,"Bas",null,"10:05","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.74,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/04/2014","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"75","GP 22","CMF 57512 DIN 75","Manuel",null,null,"Oui",1,60,2,"Non",null,null,null,5.16,2,12,"REC","REC  215 AE","Poly",2.5,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,9,null,null,null,322,112,"10:17",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais",null,"Bon",{"$nulls":9},4,0,10,40,null,32,"3*35","4*16",null,2,2,2,2,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,45,30,30,30,15,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,1,1,1,null,"Non","Non","Non","Non","Non","Non",9,null,24,null,"Non",null,null,"Non"]
["P55","0922030303700","11/07/2020","FATICK","FOUNDIOUGNE","NIORO ALASSANE TALL","NDIAYENE KAD",103,930,2020,"01/03/2015","01/06/2020",0,"SALENSOL","ERSEN II",15,6,7,4,32,"MOMATH DIBA",781653762,"ELECTRICIEN","Oui","Oui",null,"Non",368842,1533622,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",17,17,15.5,15.5,1.7,1.7,"Non","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},7.3,6.25,"Oui","Bon état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,2.6,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000 TL -20",1,5,1,5,47.7,365,{"$nulls":8},41,63,175,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Non Fonctionnel","A remplacer","Fonctionnel",null,"Oui",4,null,null,4.0999999999999996,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,null,1.23,47.7,31,30,"Bas",null,"09:12","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.65,2.6,2.25,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/03/2015","Fonctionnel",{"$nulls":10},22,400,50,20,null,null,null,"GP 22",null,"Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":4},1,365,466,"09:20",null,"Bois","LBC","Bon",null,"Bon",null,null,null,"Mauvais","A réparer",{"$nulls":8},8,0,10,40,340,32,"3*35","4*16","32 POTEAUX DONT 5 JUMELES ET 2 CONTRE FICHES",30,30,30,30,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,30,5,5,2,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,1,1,null,null,"Non","Non","Non","Non","Non","Non",null,1,24,1,"Non",null,null,"Non"]
["P56","0922030100700","11/07/2020","FATICK","FOUNDIOUGNE","KEUR S.DIANE","KERE",113,1114,2020,"01/02/2014",0,24,"SALENSOL","ERSEN II",13,10,null,4,27,"MOMATH TOURE",775528219,"ENSEIGNANT ALPHABETISATION","Oui","Non",null,null,366944,1524392,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18.600000000000001,30,17.5,30,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,"Autre","GRLLAGE ET SERRURE",7.2,6.7,"Oui","Bon état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,null,"SERRURE",null,null,null,2.75,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SIB OH 12","SMA 5000 TL 120",1,6,1,5,50.5,309,3,1.5,230,230,50,50,null,null,41,63,125,550,null,120,null,22,202,253,180,250,10,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"10/10/2017",null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,96,1.22,50.5,33,30.1,"Equilibré",null,"16:56","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.76,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/02/2014","Non Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"70","GP 22","GOUDION","Manuel","Non",null,"Oui",{"$nulls":7},5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":4},1,295,52,"17:07",null,"Bétons","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais",{"$nulls":7},8,null,null,null,8,40,1200,54,"3*35","4*16","54 POTEAUX DONT 2 CONTRE FICHES ET 2 JUMELES",4,4,4,4,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,30,30,30,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,1,null,null,null,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P57","0922030101000","11/07/2020","FATICK","FOUNDIOUGNE","Keur S. Diané","KEUR BABOU NDITY",57,990,2020,"01/01/2014",0,3,"SALENSOL","ERSEN II",19,2,2,5,28,"BABACAR GUEYE",778328555,"CHAUFFEUR","Oui","Oui",null,"Non",361794,1524226,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,30,17,30,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer","Bon Etat",null,35,null,null,null,7.5,6.2,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état","Mauvais état",null,"1 FEUILLE","SERRURE",null,null,"EXTERIEUR",2.7,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA S18 OH-12","SMA SB 5000 TL -20",1,6,1,5,50.1,300,1.8,10.4,231,231,50.1,50,null,null,41,63,125,550,null,120,null,22,202,253,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"2 FEUILLES","SERRURE",{"$nulls":5},"100 PZS 1000","HOPPECKE",24,48,2,1000,55,20,75,1.23,50.1,32.700000000000003,33.1,"Equilibré",null,"15:30","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.71,2.66,2.6,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/02/2014","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"150","GP 22","CMF 60012 DIN 100","Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",{"$nulls":5},1,350,525,"15:42",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A réparer",{"$nulls":6},1,null,1,0,8,44,600,36,"3*35","4*16","36 POTEAUX DONT 5 CONTRE FICHE",4,1,2,1,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,30,30,20,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,2,1,2,null,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["P58","1422010200200","10/07/2020","SEDHIOU","BOUNKELING","TANKON","BAMBADALA",125,3424,2019,"01/01/2014",0,12,"Energie R","ERSEN II",26,5,6,4,41,"SAMBA SOW",785226080,"ARABE","Non","Non",20000,"Non",237604,1630620,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",22.9,22.9,18.899999999999999,18.899999999999999,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",7,2,"Serrure",null,8,6.7,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"CF LOCAL BATTERIE",{"$nulls":4},3.2,2.96,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SUNNY ISLAND SI 5048","SUNNY BOY",1,5,2,5,48.6,280,null,5.8,230,230,50,50,null,null,41,63,224,480,21,120,20,22,202,253,220,280,45,65,50,60,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,3,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"9 OPZS SOLAR POWER 1370","HOPPECKE / BAE / ROLLS",24,48,2,1370,45,20,null,null,48.6,27,31,"Equilibré","01/12/2019","12:30","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",3.3,3.3,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":8},"Bon","GREEN POWER","01/01/2014","Fonctionnel",null,812,30,52,230,0,62,12,13.9,100,30,230,50,30.5,null,12,"100","ECP 28 VL4","MF DIN 100","Manuel","Non",null,"Oui",1,50,1,"Non",null,null,null,7.44,3,2,"TENESOL  / CANADIAN SOLAR","CS 6P-230P  . TE 140-36P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},875,null,null,null,"LED","Bon",null,"Bon",null,"A remplacer",null,"A remplacer",{"$nulls":7},1,1,null,0,8,40,1000,46,"4*16",null,"LE SYSTEME DE STOCKAGE EST CONSTITUE DE 3 MARQUES : HOPPECKE . BAE . ET ROLLS ET 4 TYPES DE BATTERIES SOLAR POWER 1370 10 PVV 1550 10 PVS 1500 ET 2KS 33P: ON NOTE DONC UNE HETEROGENEITE DES BATTRIES DU SYSTEME",4,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,15,30,2,15,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},1,1,1,"Non","Non","Non","Non","Non","Non",null,1,12,null,"Oui","LOCAL BATTERIE","LOCAL OPERATEUR ENERGIE R"]
["P59","1422010201900","10/07/2020","SEDHIOU","BOUNKELING","TANKON","KOHEL MOUNKOUTALLA",75,1180,2019,"01/01/2014",0,6,"Energie R","ERSEN II",33,7,1,2,43,"TAFSIR CISSE",781069032,"ARABE","Oui","Non",10000,"Non",448988,1474046,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,12,null,null,null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"CF LOCAL GE",{"$nulls":4},2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL -20",1,5,1,5,52.6,288,null,5.3,232,232,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"90 OPZS SOLAR POWER 1370","HOPPECKE",24,48,2,1370,45,20,92,1.2,49.7,30,32,"Haut",null,"16:00","Bon Etat","Bon Etat","Bon Etat","Bon Etat",3.1,2.9,3,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"ETANCHEITE TOITURE A FAIRE",{"$nulls":5},"Bon","GREEN POWER","01/01/2014","Fonctionnel",null,152.80000000000001,30,52,230,5.2,58,16,14.1,97,30,230,50,30.5,null,12,"97","GP 22","8G 30 H","Manuel","Non",null,"Oui",1,30,1,"Non",null,null,null,5.6,2,11,"CANADIAN SOLAR","CS6P -230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},409,"16:15",null,"Bois","LED","Bon",null,"Bon",null,"A remplacer",null,"A remplacer",{"$nulls":7},1,1,null,0,11,40,600,40,"3*35",null,"PROBLEME D'ETANCHEITE",4,1,2,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,30,15,30,2,15,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Oui","LOCAL BATTERIE","LOCAL ENERGIE","Non"]
["P60","1422010203400","11/07/2020","SEDHIOU","BOUNKELING","TANKON","SACITA FARYMBOURE",87,1200,2019,"01/01/2014",0,7,"Energie R","ERSEN II",33,3,2,2,40,"SEYDI DIA",776407513,"ARABE","Oui","Non",10000,"Non",451426,1471417,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",16.18,16.18,16,16,2.1,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,6,null,null,null,7.55,5.75,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL -20",1,5,1,5,52.3,272,5,9.3000000000000007,232,232,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,68,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"9 OPZS SOLAR POWER 1370 / 2KS33P","HOPPECKE / ROLLS",24,48,2,1370,45,20,null,null,52.5,27,29,"Equilibré","01/12/2019","09:40","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.5,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER","01/01/2014","Fonctionnel",null,103.6,6,52,231,5.2,47,21,14.2,null,30,230,50,30.5,null,12,"100","GP 22","DIN 100 MF","Manuel","Non",null,"Oui",1,30,1,"Non",null,null,null,5.6,2,11,"CANADIAN SOLAR","CS6P - 230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},857,"10:30",null,"Bois","LED","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":8},2,null,null,10,40,600,50,"3*35",null,null,4,1,2,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,10,15,10,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Oui","LOCAL BATTERIES","AU NIVEAU DE L'OPERATEUR ENERGIE R","Non"]
["P61","1422010204300","11/07/2020","SEDHIOU","BOUNKELING","TANKON","SARRE BOCAR",55,1000,2019,"01/01/2014",0,6,"Energie R","ERSEN II",12,7,3,2,24,"MOUSSA NIANG",781795156,"ARABE","Oui","Oui",10000,"Non",453223,1467106,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},7.54,5.7,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"CF LOCAL ONDULEUR",null,null,null,2.75,2.48,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000 TL - 20",1,5,1,5,57.9,null,14,null,260,260,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.25,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"9 OPZS SOLAR POWER 1370 . 2 KS 33P","HOPPECKE . ROLLS",24,55,2,1370,45,20,87,null,57.9,27,29,"Equilibré",null,"13:00","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.8,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER",null,"Non Fonctionnel","01/01/2014",{"$nulls":9},30,230,50,30.5,null,12,"100","GP 22","DIN 100 MF","Manuel","Non",{"$nulls":9},5.6,2,11,"CANADIAN SOLAR","CS 6P-230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},1176,"12:30",null,"Bois","LED","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},3,9,40,100,29,"3*35",null,"SEUL LE GPV FONCTIONNE. LE GE N'ESTNPAS FONCTIONNEL DEPUIS SON INSTALLATION",4,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,15,30,2,15,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},1,1,1,null,"Non","Non","Non","Non","Non",{"$nulls":4},"Oui","LOCAL BATTERIE","LOCAL SIEGE OPERATEUR ENERGIE R","Non"]
["P62","1422020300600","11/07/2020","SEDHIOU","BOUNKELING","INOR","BISSARY KANSOYE",32,1000,2019,"01/01/2014",0,8,"Energie R","ERSEN II",16,9,11,3,39,"EL HADJ IBRAHIMA SANE",772382682,"3é SECONDAIRE","Oui","Non",20000,"Oui",415956,1433279,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,36.4,null,null,null,7.6,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.7,2.5,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL -20",1,5,1,5,49.3,null,null,0.2,233,233,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",3,null,null,4.2,2.5,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"9 OPZS SOLAR POWER 1370 . 2KS 33P","HOPPECKE . ROLLS",24,48,2,1370,45,20,96,null,49.3,25,33,"Bas","01/03/2020","16:10","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.8,2.8,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER","01/01/2014","Non Fonctionnel","06/07/2020",{"$nulls":9},30,230,50,30.5,null,null,null,"GP 22","PAS DE BATTERIE","Manuel","Non",null,"Oui",1,40,3,"Non",null,null,null,5.0599999999999996,2,11,"CANADIAN SOLAR","CS6P-230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},16,null,null,"Bois","LED","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},10,0,40,600,24,"3*35",null,"LE GE NE FONCTIONNE PAS POUR DES PROBLEMES DE DEFAILLANCE DE LA BATTERIE DE DEMARAGE. SEUL LE GPV FONCTIONNE DE 10H A 20H PAR JOUR",8,1,1,1,1,"Oui",null,"Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,3,null,10,1,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},1,1,null,"Non",{"$nulls":9},"Oui","LOCAL BATTERIE","LOCAL OPERATEUR ENERGIE R","Non"]
["P63","MAG","12/07/2020","SEDHIOU","BOUNKELING","INOR","MAGNORA",20,1200,2019,"01/01/2014",0,11,"Energie R","ERSEN II",10,4,3,2,19,"OUMAR DIEDHIOU",782213621,"ARABE","Non","Non",10000,"Non",424904,1438359,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},7.54,5.75,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"CF LOCAL GE",{"$nulls":4},2.7,2.5,2.75,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL  -20",1,5,1,5,51.8,290,null,2.1,231,231,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,2.75,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"9 OPZS SOLAR POWER 1370","HOPPECKE",24,48,2,1370,45,20,19,1.22,51.8,24,26,"Bas",null,"09:25","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.5,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"2 ARDOISES A REMPLACER",{"$nulls":5},"Bon","GREEN POWER","01/01/2014","Non Fonctionnel",{"$nulls":15},12,"160","GP 22","US 12-160","Manuel","Non",null,"Oui",1,30,130,"Non",null,null,null,5.6,2,11,"CANADIAN SOLAR","CS 6P-230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":6},215,"09:20",null,"Bois","LED","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":10},0,6,40,100,12,"3*35",null,"SEUL LE GPV FONCTIONNE DE V10H A 21H",4,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,15,45,15,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},1,1,1,"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Oui","LOCAL BATTERIE","LOCAL OPERATEU ENERGIE R"]
["P64","1422020400700","12/07/2020","SEDHIOU","BOUNKELING","KANDION MANGANA","KANDION MANGANA",33,700,2017,"01/01/2012","01/01/2019",0,"Sud Solar System","ERSEN II",15,2,1,5,23,"MALANG SAGNA",785510058,"3é SECONDAIRE","Non","Non",20000,"Oui",414967,1458486,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,18,18,2,null,"Oui","Grillage","Fer",null,null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",5,3,null,null,7.5,5.75,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"A réparer",null,null,null,"CF LOCAUX ONDULEURS ET BATTERIES",null,null,"CF LOCAUX ONDULEURS ET BATTERIS",2.7,2.5,2.8,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REFAIRE","",null,"SERRURE A REMPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 80-12","SB 5000 TL -20",1,5,1,5,54,250,8.6999999999999993,12.7,230,230,50,50,null,null,41,63,175,440,26,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4.25,2.4700000000000002,2.75,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A REMPLACER","",null,"A REFAIRE",null,null,"10 OPZS 1000",null,21,42,2,1000,45,20,null,1.26,null,27,72,"Bas","01/04/2020","13:10","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"A remplacer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"A REFAIRE",{"$nulls":4},"Mauvais","GREEN POWER","01/01/2012","Non Fonctionnel","01/01/2012",{"$nulls":16},"GP 22","PAS DE BATTERIE","Manuel","Non",null,"Non",{"$nulls":5},8,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},323,null,null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"A réparer",{"$nulls":7},2,null,null,5,5,36,1800,31,"3*35",null,"L'ELECTROLYTE DES BATTERIES EST EN DESSOUS DU NIVEAU MIN",{"$nulls":10},"Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":8},"Non","Non","Non","Non","Non",3,0,24,0,"Oui","LOCAL BATTERIE",null,"Non"]
["P65","1422010300800","12/07/2020","SEDHIOU","BOUNKELING","Djinani","DJINANI",52,600,2019,"01/01/2012",0,5,"Sud Solar System","ERSEN II",4,6,8,12,30,null,779166562,null,"Non","Non",10000,null,null,null,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18,18,18,18,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",36,7,"Serrure",null,7.5,5.8,"Oui","Mauvais état",null,"Bon état",null,"Mauvais état","A réparer","Bon état",null,"Mauvais état","A remplacer","Bon état",null,"CF LOCAL ONDULEUR",null,"CF LOCAUX ONDULEURS ET BATTERIES",null,"CF LOCAUX ONDULEURS ET BATTERIES",null,2.7,2.5,2.75,"Bon Etat",null,"Bon Etat",null,"Bon Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"A réparer",{"$nulls":4},"FISSURES A REPARER",null,null,"SERRURE A REMPLACER",null,"A REPRENDRE",{"$nulls":37},"A remplacer",null,"A remplacer",null,"Non",null,null,null,4.3,2.5,2.75,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A REMPLACER",null,"A FAIRE",{"$nulls":19},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER",{"$nulls":12},25,230,50,25.6,null,12,"100","GP 22","DIN 100 MF","Manuel","Non",{"$nulls":9},5.16,null,null,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.7,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},"Bon",{"$nulls":35},"SEULLA PARTIE GE FONCTIONNE ET IL EST GERE PAR LA POPULATION. LA PARTIE PV NE FONCTIONNE PAS . LES MODULES PV SONT DECONNECTES",{"$nulls":57},2,24,1,"Oui","LOCAL BATTERIES",null,"Non"]
["P66","1422010301300","12/07/2020","SEDHIOU","BOUNKELING","Djinani","MANSABANG",62,750,2019,"01/01/2012","01/05/2020",0,"Sud Solar System","ERSEN II",5,7,7,4,23,"SOUKAROU CAMARA",774963687,"3é SECONDAIRE","Non","Non",10000,"Non",414960,1458489,"Solaire_GE","Non","Non Inondable","Délibération","Oui",17,17,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",66,2,null,null,7.5,6,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Mauvais état",null,"Bon état",null,"A réparer",null,null,null,"SERRURE A REMPLACER",null,null,"A REPRENDRE",2.8,2.5,3,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REPRENDRE",null,null,"SERRURE A REMPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8.0 H-12","SB 5000 TL-21",1,6,1,5,{"$nulls":10},41,63,175,440,26,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",2,"01/12/2018",null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A REMPLACER",null,null,"A REPRENDRE",null,null,"10 OPZS 1000","HOPPECKE",21,42,2,1000,45,-20,null,null,41.2,{"$nulls":5},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",3,3,2.6,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"A REPRENDRE",{"$nulls":4},"Bon","GREEN POWER","01/01/2012","Non Fonctionnel","01/12/2019",{"$nulls":9},25,230,50,25.5,null,12,"75","GP 22","MF DIN 75","Manuel","Non",null,"Non",null,null,null,"Non",null,null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,2,{"$nulls":4},410,null,null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},6,0,40,1850,14,"3*35",null,"ARRET COMPLET DE LA CENTRALE DEPUIS FEVRIER 2020",2,1,1,1,1,"Oui","Oui","Non","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,1,30,1,1,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Sous traitant",null,null,"Opérateur",null,null,72,72,72,48,1,"Non","Non","Non","Non","Non","Non",2,null,24,null,"Oui","LOCAL BATTERIES","SIEGE SUD SOLAR A ZIGUINCHOR"]
["P67","1422010403100","13/07/2020","SEDHIOU","BOUNKELING","NDIAMALATHIEL","VELINGARA SARE YAYA 3",57,779,2019,"01/01/2014","01/07/2020",0,"Sud Solar System","ERSEN II",15,1,0,4,20,"ABDOULAYE DIOP",781282184,"ARABE","Non","Non",10000,"Non",419674,1470190,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,20,null,null,null,7.8,5.8,"Oui","Bon état",null,"Mauvais état","A remplacer","A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"A REMPLACER LOCAUX ONDULEURS ET BATTERIES","SERRURE A CHANGER",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"A REPRENDRE",{"$nulls":4},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL-20",1,5,1,5,{"$nulls":10},41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.3,2.5,3,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A CHANGER",{"$nulls":5},"9 OPZS SOLAR POWER 1370","HOPPECKE",22,44,2,1370,45,-20,{"$nulls":8},"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,2.5,2.6,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REMPLACER",{"$nulls":5},"Bon","CUMMINS","01/01/2014","Non Fonctionnel",{"$nulls":10},22,400,50,{"$nulls":4},"C 22 D5",null,"Manuel","Non",null,"Non",null,null,null,"Non",null,6,null,5.6,2,11,"CANADIAN SOLAR","CS 6 P-230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,"Bon",{"$nulls":6},411,"09:50",null,"Bois","LBC","Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":7},1,null,null,8,0,45,830,26,"3*35",null,null,2,1,1,null,1,"Oui","Oui","Non","Non","Oui","Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,15,30,null,15,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":5},"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",null,null,24,null,"Oui","LOCAL BATTERIE","SIEGE SUD SOLAR SYSTEM"]
["P68","0622030302800","19/07/2020","KAOLACK","NIORO","WACK NGOUNA","KEUR NDONGO",59,600,2019,"01/01/2013",0,8,"Energie R","ERSEN II",25,4,1,1,31,"MAMADOU NDIAYE",771581987,"CM1","Non","Non",15000,"Non",388797,1517241,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",70,3,null,null,7.5,5.8,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"CF LOCAUX ONDULEURS BATTERIES ET GE",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL -20",1,5,1,5,49.4,255,11,16.899999999999999,230,230,50,50,null,null,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/01/2018",null,4.25,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A CHANGER",{"$nulls":5},"10 OPZS 1000","HOPPECKE",23,46,2,1000,45,-20,74,1.25,49.4,28,30,"Bas","01/01/2019","14:30","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,"Bon","GREEN POWER","01/01/2013","Non Fonctionnel",{"$nulls":10},25,230,50,25.5,null,12,"75","GP 22","MF DIN 75","Manuel","Non",null,"Oui",1,30,30,"Non",{"$nulls":4},2,12,"REC  SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"A réparer",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,2,{"$nulls":4},900,"14:35",null,null,"LBC","Bon",null,"Bon",null,"A remplacer",null,"A réparer",{"$nulls":7},1,null,null,null,10,40,400,24,"3*35",null,"2 MODULES PV SONT CASSES . FONCTIONNEMENT UNIQUEMENT AVEC LE GPV DE 15H A 23H",2,1,1,1,1,"Oui","Oui","Non","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,30,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",2,null,2,null,"Non",null,"LOCAL BATTERIE","Non"]
["P69","0622030105300","20/07/2020","KAOLACK","NIORO","KEUR MABA DIAKHOU","THYLLA GRAND",89,1266,2019,"01/01/2009","2018-01-01",0,"Energie R","ERSEN I",{"$nulls":5},"BAYE NIASS NDIAYE",779359899,"ARABE","Non","Non",null,null,399972,1505539,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,20,15,15,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",15,2,"Serrure",null,8,5,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.7,2.5,3.17,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Réseau",null,"Monophasé","Monophasé",null,"SB 5000 TL -20",null,null,1,5,{"$nulls":12},175,440,null,null,20,22,null,null,180,280,null,null,45,65,"A remplacer",null,"Non Fonctionnel",null,"Non",null,null,null,4,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"A REMPLACER","SERRURE A REPRENDRE",{"$nulls":18},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.5,2.5,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Mauvais","CUMMINS","01/01/2009","Non Fonctionnel","01/01/2011",{"$nulls":9},22,400,50,{"$nulls":4},"C22D5",null,"Automatique","Non",null,"Non",{"$nulls":7},5.0999999999999996,null,null,"SCHOTT SOLAR","ASE -165-GT-FT/MCI","Poly",170,4.78,35.5,44,5.3,"A réparer",null,"Bon",null,"A remplacer",null,"A réparer",null,"Bon",null,"A réparer",null,"A remplacer",null,"Bon",null,1,{"$nulls":7},"Bois","LBC",{"$nulls":24},"ARRET DE LA CENTRALE DEPUIS 2015 . CENTRALE ABANDONNEE DEPUIS 2016 SANS SURVEILLANCE. LE VILLAGE EST ALIMENTE PAR LA SENELEC DEPUIS JANVIER 2018",{"$nulls":56},1,null,24,1,"Non"]
["P70","0622030103000","20/07/2020","KAOLACK","NIORO","KEUR MABA DIAKHOU","NAOULEROU",89,750,2019,"01/01/2009","2018-01-01",0,"Energie R","ERSEN I",{"$nulls":5},"MATAR DRAME",775892119,"ARABE","Non","Non",10000,"Oui",399572,1503596,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,20,16,16,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",72,4,null,null,5.8,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"A réparer",null,"Mauvais état","A remplacer",null,"CF LOCAUX ONDULEURS ET GE","CF LOCAUX ONDULEURS BATTERIES ET GE",null,"CF LOCAUX ONDULEURSE ET BATTERIES","CF LOCAUX ONDULEURS ET BATTERIES",2.8,2.2999999999999998,3,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","A réparer",null,"A réparer",null,"Bon Etat",null,"A réparer",{"$nulls":4},"A NREPRENDRE",null,"A REPRENDRE","SERRURE A REMPLACER",null,"A REFAIRE",null,"Onduleur Chargeur",null,"Monophasé",null,"HP-COMPACT 6000 -48",null,1,6,{"$nulls":12},38,68,null,null,1,30,null,null,230,253,null,null,49.95,50.05,null,null,"Non Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,3.35,2.8,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE",null,"A REFAIRE","A REFAIRE",{"$nulls":18},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.88,2.2999999999999998,2.7,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"A REPRENDRE",null,null,"SERRURE A REMPLACER",null,null,"Bon","CUMMINS","12/01/2009","Non Fonctionnel","01/01/2012",{"$nulls":9},22,400,50,{"$nulls":4},"C22 D5",{"$nulls":12},5.0999999999999996,null,null,"SCHOTT _ SOLAR","ASE - 165 -GT- FT/MCI","Poly",170,4.78,35.5,44,5.3,"A réparer",null,"Bon",null,"A remplacer",null,"A remplacer",null,"Bon",null,"A remplacer",null,"A remplacer",null,"Bon",null,3,{"$nulls":33},"ARRET COMPLET DE LA CENTRALE DEPUIS 2014 . VILLAGE ALIMENTE PAR LA SENELEC DEPUIS 2018",4,1,1,1,1,{"$nulls":5},"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,30,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non",{"$nulls":5},3,2,24,1,"Non",{"$nulls":4},"LES LOCAUX BATTERIES ET ONDULEURS SONT OCCUPES PAR BOUBACAR BA ET ALIOU BOUSSO"]
["P71","0622010101500","21/07/2020","KAOLACK","NIORO","KAYEMOR","PADAF",98,1460,2019,"01/01/2014",0,24,"Energie R","ERSEN II",19,8,0,3,30,"BABACAR DIALLO",782824229,"ARABE","Oui","Non",15000,"Oui",399965,1505549,"Solaire_GE","Oui","Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",70,2,"Serrure",null,7.5,5.8,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"CF LOCAUX BATTERIE ET GE",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8.O H-12","SB 5000 TL -20",1,6,1,5,50.3,295,4.5,7.1,230,230,50,50,null,null,41,63,175,440,16,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/01/2018",null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A CHANGER",{"$nulls":5},"10 OPZS 1000","HOPPECKE",22,44,2,1000,45,-20,null,1.21,50.3,25,27,"Haut",null,"10:15","Bon Etat","Bon Etat","Mauvais Etat","Bon Etat",2.7,2.7,2.75,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,"Bon","GREEN POWER","01/01/2014","Non Fonctionnel","01/03/2020",{"$nulls":9},25,230,50,25.5,null,12,"100","GP 22","6 FM 100","Manuel","Non",null,"Oui",1,20,30,"Non",{"$nulls":4},2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,2,{"$nulls":4},572,"10:25",null,null,"LBC","Bon",null,"Bon",null,"A remplacer",null,"A réparer",{"$nulls":7},2,null,null,8,2,35,550,58,"3*35",null,"FONCTIONNE UNIQUEMENT AVEC LE GPV 24H/24H. 2 MODULES PV SONT CASSES . LA BATTERIE DE DEMARAGE DU GE EST HS DEPUIS MARS 2020 . LES ABONNES UTULISENT DES COMPTEURS PREPAIEMENT AVEC TOUJOUR DES ABONNEMENTS PAR NIVEAU DE SERVICE",4,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,30,null,40,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",2,null,2,null,"Oui","LOCAL BATTERIE",null,null,null,"CERTAINS RUBRIQUES SUR LA MAINTENACE DES EQUIPEMENTS ET LA GESTION DES DECHETS N'ONT PAS PU ETRE RENSEIGNEES FAUTE DE REPONDANT DU COTE DE L'OPERATEUR"]
["P72","0632010200800","17/07/2020","KAOLACK","GUINGUINEO","NDIAGO","NDIAGNE KAHONE",41,611,2019,"01/01/2009","01/01/2015",0,"NS RESIF","ERSEN I",19,1,0,6,29,"MODY DIALLO",775255137,"ARABE","Non","Non",10000,"Oui",411358,1586852,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,20,15,15,3,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",70,12,null,null,5.8,5.7,"Oui","Mauvais état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,"CF LMOCAL BATTERIE","CF LOCAL BATTERIE",null,null,"CF LOCAUX ONDULEURS ET BATTERIES",null,2.5,1.75,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":8},"A REPRENDRE",null,"Onduleur Chargeur",null,"Monophasé",null,"HP-COMPACT6000",null,1,5,{"$nulls":12},38,68,null,null,1,30,null,null,230,253,null,null,49.95,50.05,null,null,"Non Fonctionnel",null,"A remplacer",null,"Oui",2,null,null,3.4,2.5,2.9,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A RESTAURER","A REPRENDRE",{"$nulls":6},"8 OPZS 800","HOPPECKE",21,42,2,800,45,-20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",2.7,2,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Mauvais","CUMMINS","01/01/2009","Non Fonctionnel","01/01/2015",{"$nulls":9},11,400,50,{"$nulls":4},"C 11 D5",null,"Automatique","Non",null,"Oui",1,20,null,"Non",null,null,null,4.25,null,null,"SCHOTT SOLAR","ASE -165-GT-FT-/MCI","Poly",170,4.71,36,44,5.25,"A réparer",null,"Bon",null,"A remplacer",null,"A réparer",null,"Mauvais",null,"Mauvais",null,"A remplacer",null,"Bon",null,2,{"$nulls":7},"Bois","LBC","Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":9},1,0,4,40,2500,19,"3*35",null,"VOL DE 2 MODULES PV . CENTRALE A L'ARRET DEPUIS 2015",8,1,1,1,1,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",2,2,24,1,"Oui","LOCAL BATTERIE",null,"Non"]
["P73","0632010200700","17/07/2020","KAOLACK","GUINGUINEO","NDIAGO","NDELLE",100,1334,2019,"01/01/2008","01/01/2005",0,"Energie R","ERSEN I",7,11,4,6,28,"EL HADJ DIOUF",775469172,"ARABE","Non","Non",null,null,410117,1577595,"Solaire_GE","Non","Non Inondable","Délibération","Oui",29.8,29.8,28.8,28.8,2,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",117,47,"Autre","PORTE CENTRALE",6.35,2.77,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"CF LOCAUX ONDULEURS ET BATTERIES",null,null,null,2.4,2.7,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000 TL -20",2,10,4,5,{"$nulls":10},41,63,null,null,21,120,null,null,202,253,null,null,45,65,null,null,"Non Fonctionnel",null,"Non Fonctionnel",null,"Non",null,null,null,4,2.7,2.8,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"SERRURE A CHANGER",{"$nulls":5},"16 OPZS 2000","HOPPECKE",24,48,2,2000,45,-20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",null,null,null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":44},14.26,null,null,"PV - MODUL REC SOLAR","P110/6+ REC 215 AE","Poly",130,7.3,18,22.1,7.8,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"A réparer",null,"A remplacer",null,"A réparer",{"$nulls":9},"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":10},14,1,40,700,87,"3*35",null,"ARRET COMPLET DE LA CENTRALE EN DEBUT 2016",{"$nulls":58},245,1,"Non",null,null,"Non"]
["D1","1432030200400","14/07/2020","SEDHIOU","GOUDOMP","SIMBANDI BRASSOU","BISSASSOU DOUMA",66,926,2020,"01/01/2012","2020-04-01",0,"Sud Solar System","ERSEN II",16,4,6,1,27,"AMATA NGAHBO",772064483,"PAS DE NIVEAU","Non","Non",20000,"Oui",453352,1391241,"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",19,19,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",72,28,"Serrure",null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"5 ARDOISES FIBROCIMENT","3 CERRURES A CHANGER",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"2 ARDOISES A REMPLACER","1 CERRURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI.5048","SB 5000TL 20",1,5,1,5,{"$nulls":10},41,63,175,400,217,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"1 CERRURE A REMPLACER",null,"A REPRENDRE",null,null,null,"10 OPZS 1000","HOPPECKER",21,5,2,1000,{"$nulls":7},"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.6,2.6,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"3 ARDOISE FIBROCIMENT",null,null,"1 CERRURE A CHANGER",null,null,"Bon","GREEN POWER - GP 22","01/01/2012","Non Fonctionnel","01/01/2015",{"$nulls":10},240,50,15,null,198,"75","GREEN POWER GP 22","GOUDRON","Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,4730,2,11,"REC","REC 215 AE",null,215,7.5,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"A remplacer",null,"Bon",{"$nulls":9},2,null,null,null,280,23,"13:40",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},8,8,40,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},34,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,{"$nulls":4},"Non","Non","Non","Non","Non","Non",2,null,3,null,"Non",null,null,"Non"]
["D2","1432030200500","14/07/2020","SEDHIOU","GOUDOMP","SIMBANDI BRASSOU","BISSADOU SANTO",97,1194,2020,"01/01/2014",0,1,"Sud Solar System","ERSEN II",16,7,12,2,37,"ALPHOUSSEYNOU DIASSY",773221828,"ARABE","Non","Non",20000,"Oui",453392,1392622,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",19,19,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"Serrure",null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"8 ARDOISES FIBROCIMENT","2 CERRURES",null,"A REPRENDRE",null,2.75,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A réparer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":5},"1 ARDOISE FIBROCIMENT","1 CERRURE",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8 OH - 12","SB5000M-20",1,5,1,5,51.3,259,16,4.3,null,231,{"$nulls":4},41,63,175,400,26,120,15,30,230,253,220,240,45,65,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,"01/01/2019",4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"07","UNE CERRURE",null,"A REPRENDRE",null,null,null,"OPZS SOLAR POWER","HORPECKE",22,51,2,1370,{"$nulls":4},51.3,null,null,"Bas",null,"12:22","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.75,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":8},"Bon","GREEN POWER GP 22","01/01/2014",{"$nulls":12},240,50,15,null,12,"75","GP 22","ZAHE","Manuel","Non",null,"Oui",1,40,null,"Non",null,null,null,5060,2,11,"GANDIAN SODAR","CS6P - 23OP","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,"Bon",{"$nulls":5},279,16,"12:30",{"$nulls":20},8,8,35,null,null,"4*16",null,null,2,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},34,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",null,null,2,null,"Non",null,null,"Non"]
["D3","1432010101600","13/07/2020","SEDHIOU","GOUDOMP","DJIBANAR","KLONYA",25,1420,2020,"01/01/2014",0,2,"NS RESIF","ERSEN II",3,3,null,1,7,"OUSMANE MANE",782377101,"CM2","Non","Oui",10000,"Oui",410682,1381385,"Solaire_GE","oui","Non Inondable","Délibération","Oui",19,19,16,16,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Bon Etat",null,70,null,"Serrure",null,7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"ETANCHEITE  - LOCAL ONDULEUR","1 PORTE CERRURE A CHANGER",null,"A PEINDRE",null,2.75,2.5,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"A réparer",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",{"$nulls":4},"ETANCHEITE A VOISIN","CERRURE A CHANGER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048 SMA","SB 5000TL 20 SMA",1,5,1,5,55.7,304,4.8099999999999996,74,229.9,230,49.99,null,11,11,41,63,175,400,21.7,120,15,30,230,253,220,240,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,null,null,4.2,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,"A REPARER","CERRURE A REMPLACER",null,"A REPRENDRE","A BOUCHER",null,null,"10 OPZS 1000 Au","HOPPECKE",22,55,2,1000,null,null,83.8,null,48,null,71.099999999999994,"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.75,2.65,2.6,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"1 FIBROCIMENT A CHANGER",{"$nulls":5},"Bon","GREEN POWER GP 22","01/01/2014","Fonctionnel",{"$nulls":11},240,50,15,null,null,null,"GP 22","NEANT","Manuel","Non",null,"Non",null,null,null,"Oui",null,null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.6,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":7},"Bon",{"$nulls":9},"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"A remplacer",{"$nulls":8},1,null,10,1,null,null,null,"4*16",null,null,3,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":19},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,5,{"$nulls":4},"Non","Non","Non","Non","Non","Non",null,2,2,null,"Non",null,null,"Non"]
["D4","1432010100600","12/07/2020","SEDHIOU","GOUDOMP","DJIBANAR","BAFATA BALANTE",99,1400,2020,"01/01/2014","01/12/2019",0,"NS RESIF","ERSEN I",12,11,3,1,27,"ALPHOUSSEYNOU MANSSALY",783288862,"PAS DE QUALIFICATION","Non","Non",5000,"Oui",409712,1377742,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,18,18,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",72,24,"Autre","CROCHET ET CADENAS",7.5,5.5,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,"4 FIBROCIMENT A CHANGER","2 CERRURES A CHANGER",null,"A REPRENDRE",null,2.5,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"A réparer",{"$nulls":7},"1 CERRURE A REMPLACER",null,"A REPRENDRE",null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 804 - 12 Sunn YSLAND","SB 5000TL20 SMA",1,5,1,5,{"$nulls":10},41,63,175,400,26,120,15,30,230,253,220,240,45,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",2,"01/01/2017",null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"3 ARDOISE FIBROCIMENT","1 CERRURE A REMPLACER",null,"A REPRENDRE",null,null,null,"10 OPZS 1000 Au","HOPPECKE",24,48,2,1000,{"$nulls":7},"Bas",null,null,"Mauvais Etat","Bon Etat","Mauvais Etat","Mauvais Etat",2.5,2.5,2.7,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"1 ARDOISE",null,null,"CADENAS A REMPLACER",null,null,"Mauvais","GREEN POWER GP 22","01/01/2014","Non Fonctionnel","01/12/2019",{"$nulls":10},240,50,15,null,12,"100","GP - 22 - SH - PW - N - A","JARRET 100AH","Manuel","Non",null,"Oui",1,100,4,"Non",null,null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.6,28.3,36.299999999999997,8.1,"Bon",null,"Bon",null,"Bon",null,"Bon",null,null,null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},15,null,null,"Bois","LBC","Bon",null,"Bon",null,"A remplacer",null,"Mauvais",{"$nulls":7},1,7,1,7,7,40,null,null,"4*16",null,null,6,{"$nulls":4},"Oui",{"$nulls":4},"Conducteur",{"$nulls":14},2,{"$nulls":4},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,3,{"$nulls":5},"Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["D5","0922030200300","12/07/2020","FATICK","FOUNDIOUGNE","KEUR SAMBA GUEYE","DJIDA",73,730,2020,"01/08/2014","01/01/2020",0,"Sud Solar System","ERSEN II",40,0,1,4,45,"OSD THIAW",773046706,"CULTIVATEUR","Oui","Non",10000,"Oui",351661,1503402,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,null,17,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer",null,3,null,null,7,5,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,"4 FEIUILLES","CERRURE",null,null,null,2.5,2.2999999999999998,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":6},"2 FEUILLES","CERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA515045","SMA SB 5000TL- 20",1,512,1,512,41.6,332,0.4,0.4,229,229,50,50,16155,16155,41,63,125,550,null,120,null,22,172.5,246.5,180,280,45,75,45,55,"Non Fonctionnel","A remplacer","Fonctionnel",null,"Oui",4,null,null,3.5,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"1 FEUILLE","CERRURE",{"$nulls":4},"10 OPZS 10","HOPPECKE",24,48,2,1000,55,20,85,null,41.6,26.3,31.1,"Bas",null,"17:00","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.6,2.5,2.7,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"1 FEUILLE",null,null,"SERRURE",null,null,"Bon","GREEN POWER","01/08/2014","Non Fonctionnel",{"$nulls":10},22,4001230,50,20,75,null,null,"GP 22",null,"Manuel","Non",null,"Non",null,null,1,"Oui","DEBITTERMATEUR",null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",{"$nulls":5},1,307,40,"17:05",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A remplacer","Mauvais","A réparer",{"$nulls":6},2,null,11,0,10,42,720,34,"3*70","3*35",null,4,10,10,10,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,20,20,20,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,1,1,2,null,"Non","Non","Non","Non","Non",null,null,1,24,null,"Non",null,null,"Non"]
["D6","0922030201000","12/07/2020","FATICK","FOUNDIOUGNE","KEUR SAMBA GUEYE","KEUR ALLASSANE DIALLO",86,934,2020,"01/01/2014",0,3,"Sud Solar System","ERSEN II",23,7,0,4,34,"FAMARY MARONE",772548037,"CULTIVATEUR","Oui","Non",10000,"Oui",361269,1503756,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,1.7,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":5},7,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,"1 FEUILLE","SERRURE",null,null,null,2.2000000000000002,2,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMASB5000 - 20",1,5,1,5,46,231,4.5999999999999996,4.5999999999999996,230,230,50,50,14416,14416,41,63,125,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4,2,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,null,"1 FEUILLE","SERRURE",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,23,12,46,31,30.6,"Equilibré",null,"14:20","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.5,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/01/2014","Fonctionnel",{"$nulls":10},22,400,50,20,null,null,null,"GP 22",null,"Manuel","Non",null,"Oui",1,30,2,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.200000000000003,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":5},319,30,"14:30",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais","A réparer",{"$nulls":6},3,null,3,0,8,42,null,41,"2*16",null,null,4,1,3,0,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,30,2,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,null,1,2,null,null,"Oui","Non","Non","Non","Non",null,0,0,24,null,"Non",null,null,"Non"]
["D7","0922030202600","12/07/2020","FATICK","FOUNDIOUGNE","KEUR SAMBA GUEYE","MEDINA DIOGOYE",52,780,2020,"01/01/2015",0,9,"Sud Solar System","ERSEN II",28,1,1,4,34,"MOMATH SAKHO",784487710,"ELECTRO-MECANICIEN","Oui","Non",5000,"Oui",366694,1506916,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",18,null,17,null,1.5,null,"Oui","Grillage","Fer",null,null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",null,3,"Serrure",null,7,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A réparer",null,null,"SERRURE",null,null,null,2.68,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 45048","SMASB5800TL - 20",1,512,1,512,51,329,9.9,9.9,230,230,50,50,12,12,41,63,125,550,null,120,null,22,202,253,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"10 OPZS 1000","HOPPECKE",24,48,2,1000,55,20,88,2.2200000000000002,51,30.1,51.1,"Bas",null,"12:30","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.85,2.65,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEEN POWER","01/01/2015","Non Fonctionnel",{"$nulls":10},22,400,50,20,75,null,null,"GP 22",null,"Manuel","Non",null,"Oui",1,30,3,"Non",null,null,null,5.16,2,12,"REC","REDC 215 AE","Poly",215,7.7,28.2,36.200000000000003,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",{"$nulls":5},321,229,"23:41",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais",{"$nulls":7},2,null,3,0,11,42,800,40,"2*16",null,null,3,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,30,30,30,30,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":4},2,null,null,"Oui",{"$nulls":6},1,null,null,"Non",null,null,"Non"]
["D8","0912020201500","09/07/2020","FATICK","FOUNDIOUGNE","Loule Séssene","SAKHOR",145,1375,2020,"01/04/2010",0,8,"Sud Solar System","ERSEN II",35,28,27,0,90,"PHILOMENE SARR",770221147,"BACCALAUREAT ET DIRECTEUR D'ECOLE","Non","Non",5000,"Oui",335970,1573804,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",20,30,18,30,2,null,"Oui","Mur&Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,76,null,null,null,7,2.5,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer",null,"2 FEUILLE A REMPLACER","SERRURE POUR LES 3 PORETS",null,null,"A REPRENDRE",2.4,2.2999999999999998,3,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,"DALLE A REFAIRE",null,"1 FEUILLE A REMPLACER","SERRURE A REMEPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","Sunny ISLAND SI 5048","Sunny BOY SB 1700",2,5,3,1.5,46.1,192,0,1.8,230,230,50,50,16445,16445,41,63,139,400,null,120,null,8.6,172.5,264.5,180,260,40,70,45.5,54.5,"Non Fonctionnel","A remplacer","Non Fonctionnel","A remplacer","Non",null,null,null,4.3,2.4,3,"Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"1 FEUILLE A CHARGER","SERRURE",null,null,"DALLE A REPRENDRE",null,null,"10 OPZS1000","KOPPECKE",24,48,2,1000,55,20,63,1.18,44,31.5,31.5,"Equilibré",null,"17:15","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.2999999999999998,2.2000000000000002,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Mauvais","GREEN POWER",null,"Non Fonctionnel",{"$nulls":10},22,400,50,20,{"$nulls":5},"Manuel","Non",null,null,null,20,{"$nulls":5},4.76,2,17,"TENESOL","TE'40 - 36 P","Poly",140,8,17.5,22.1,8.4,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},190,630,"17:38",null,"Bois",null,"Bon",null,"Bon",null,"Mauvais",null,"Mauvais","A remplacer",{"$nulls":8},6,0,8,45,285,36,null,null,null,4,4,1,null,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,1,10,15,null,10,"Conducteur","Opérateur",null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur","Sous traitant",null,"Opérateur",null,null,1,15,2,2,0,"Non","Non","Non","Non","Non","Non",0,2,24,34,"Non",null,"OPERATEUR"]
["D9","1212020100800","17/07/2020","KAFFRINE","KOUNGHEUL","Diokoul","KATHIOLE",37,550,2020,"01/01/2014",0,11,"ERA",null,25,4,3,6,38,"L'OPERATEUR EST ERA",709303031,null,"Non","Non",null,null,464725,1550161,"Solaire","Oui","Non Inondable","Délibération","Oui",30,30,30,30,1.7,null,"Oui","Mur&Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",{"$nulls":5},6.3,3,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},4,2,2.2999999999999998,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Triphasé","SMA SI 5048","SMA STP15000TL - 10",3,5,1,15,48,728,1.78,1.78,223,223,null,null,17,null,41,63,125,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,2,1,2.2999999999999998,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":9},"10 OPZSSOLAR POWER125C","HOPPECKE",24,48,2,1350,55,20,null,null,48,23.7,24.2,"Equilibré",null,"17:10","Bon Etat","Bon Etat","Bon Etat","Bon Etat",null,null,null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":44},13.75,2,33,"SOLAR WATT","SOLAR WATT","Poly",250,8.2799999999999994,30.2,37.6,8.69,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":5},730,55,"17:05",null,"Bois",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":9},0,0,0,41,null,23,"4*16",null,"LE RESAEU COUVRE TOUT LE VILLAGE",1,1,1,null,1,"Oui","Oui","Oui","Oui","Oui","Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,24,14,11,null,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Oui","Oui","Oui","Oui",{"$nulls":5},2]
["D10","0922010100200","13/07/2020","FATICK","FOUNDIOUGNE","DJILOR","BANGALERE",74,940,2020,"01/01/2014",0,8,"Sud Solar System","ERSEN II",26,8,6,2,42,"LAMINE DIOUF",778062265,"AGRICULTEUR","Oui","Non",10000,null,346682,1543446,"Solaire_GE","Oui","Non Inondable","Non Immatriculé","Oui",17,null,16.5,null,1.7,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer",45,6,"Serrure",null,7.3,5.6,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Bon état",null,"Bon état",null,null,"SERRURE",{"$nulls":4},2.2999999999999998,2.2000000000000002,3.2,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI5048","SMA SB 5000TL20",1,5,1,5,46.2,310,11.4,11.4,230,230,50.1,50.1,9435,9435,41,63,125,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/01/2018",null,3.9,2.2000000000000002,3.2,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"2 FEUILLES",{"$nulls":6},"10OPZS 1000","HOPPECKE",24,48,2,1000,55,20,39,null,46.2,28.7,31.8,"Equilibré",null,"09:38","Mauvais Etat","Bon Etat","Bon Etat","Mauvais Etat",2.5,2.2000000000000002,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE",null,null,"Bon","GREEN POWER","01/01/2014","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"75","GP 22","GOUDRON D N75","Manuel",null,null,"Non",null,null,null,"Non",null,null,null,5.16,2,12,"REC","REC 215 AE","Poly",15,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",null,null,1,null,null,1,306,827,"09:45",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Mauvais","A réparer",{"$nulls":8},0,null,9,40,400,32,"3*70","3*35",null,8,8,8,8,null,"Oui","Oui","Oui","Oui",null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,30,30,30,30,null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur",null,null,null,30,14,30,null,"Non","Non","Non","Non","Non","Non",1,null,24,null,"Non",null,null,"Non"]
["D11","0922010203200","13/07/2020","FATICK","FOUNDIOUGNE","DIOSSONG","NDORONG SERERE",89,900,2020,"01/05/2017",0,15,"Sud Solar System","ERSEN II",42,26,4,6,78,"DIENE FAYE",773891409,"CULTIVATEUR","Oui","Non",20000,"Non",355135,1547419,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",31,31,16.5,16.5,1.7,null,"Non","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A remplacer","Bon Etat",{"$nulls":5},9.8000000000000007,5.2,"Oui","Bon état",null,"Mauvais état","A réparer","Mauvais état","A réparer","Mauvais état","A réparer","Bon état",null,"Mauvais état","A remplacer",null,null,"6 FEUILLES","SERRURES",null,null,2.5,2.2000000000000002,3,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",{"$nulls":6},"2 FEUILLES","SERRURES",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 8 04 -12","SMA SB 5000TL - 20",2,6,2,5,50,293,14.6,14.6,230,230,50,50,11,11,41,63,125,550,null,120,null,22,172.5,264.5,180,280,40,70,45,55,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/12/2018",null,5,2.2000000000000002,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"2 FEUILLES","SERRURE",{"$nulls":5},"10 OPZS1000","HOPPECKE",48,48,2,1000,55,20,null,1.18,50,30.5,31,"Bas",null,"11:30","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.5,2.5,2.5,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"2 FEUILLES",null,null,"SERRURE",null,null,"Bon","GREEN POWER","01/01/2017","Fonctionnel",{"$nulls":10},22,400,50,20,null,12,"100","GP 22","HS 100 CMF","Manuel","Non",null,"Oui",1,30,2,"Non",null,null,null,10.32,4,12,"REC","REC 215 AE","Poly",215,7.7,28.2,36.5,8.3000000000000007,"Mauvais","A réparer","Bon",null,"Mauvais","A remplacer","Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer",null,null,1,null,null,2,263,1003,"11:38",null,"Bois","LBC","Bon",null,"Bon",null,"Mauvais","A réparer","Mauvais","A réparer",{"$nulls":8},5,0,10,42,540,38,"3*70","3*35",null,3,3,0,3,null,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,"Conducteur",null,null,3,1,null,30,null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",null,"Opérateur","Sous traitant",{"$nulls":4},1,1,1,1,null,"Non","Non","Non","Non","Non","Non",61,null,48,null,"Non",null,null,"Non"]
["D12","1422010402100","13/07/2020","SEDHIOU","BOUNKELING","NDIAMALATHIEL","MISSIRA KABALOR",78,788,2019,"01/01/2013","01/07/2020",0,"Sud Solar System","ERSEN II",12,2,3,3,20,"ALPHA OUMAR DIALLO",777901878,"CM2","Non","Non",10000,"Non",419249,1471386,"Solaire_GE","Non","Non Inondable","Délibération","Oui",17,17,18,18,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer",15,1,null,null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Bon état",null,"A réparer",null,null,"LOCAUX ONDULEURS BATTRIE ET GE","LOAUX ONDULEURS",null,null,"LOCAL GE",2.8,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"A REPRENDRE","SERRURE A REMPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL - 20",1,1,1,5,47.5,{"$nulls":9},41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",4,null,null,4.3,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REPRENDRE",{"$nulls":6},"90PZS SOLAR - POWER 1370","HOPPECKE",24,48,2,1370,45,20,19,null,47.5,27,26,"Haut",null,"11:30","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.9,2.9,3,"Bon Etat",null,"Mauvais Etat","A remplacer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REPRENDRE","A REPARER",{"$nulls":4},"Bon","CUMMINS POWER GENERATION","01/01/2013","Non Fonctionnel","01/03/2020",{"$nulls":9},25,230,50,25.5,null,12,"75","C22D5","MF DIN75","Manuel","Non",null,"Oui",1,20,null,"Non",null,null,null,5.6,2,11,"CANADIEN SOLAR","CS6P - 23OP","Poly",30,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},877,"11:30",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},10,null,40,550,32,"3*35",null,"LES TOITURES DES LOCAUX  LES ONDULEURS  LES BATTRIES  ET GE DOIVENT ETRE RENOVES D'URGENCE",2,1,1,1,1,"Oui","Oui","Oui","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",0,2,24,0,"Oui","LOCAL BATTRIE",null,"Non"]
["D13","1422010402600","13/07/2020","SEDHIOU","GOUDOMP","BAGHERE","SARRE BITEYE",70,900,2019,"01/01/2013",0,8,"Sud Solar System","ERSEN II",19,6,3,3,31,"YAYA SY",772018925,"ARABE","Non","Non",10000,"Oui",420771,1473282,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,34,null,null,null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"LOCAUX  ONDULEURS BATTRIES GE","LOCAL ONDULEUR",null,null,null,2.7,2.4,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"A Remplacer",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"A REPRENDRE","SERRURE A REMPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SMA SI 5048","SMA SB 5000TL - 20",1,5,1,5,50.9,276,1.85,15.5,232,232,50,50,13,13,41,63,175,440,21,120,20,22,20,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",3,null,null,4.2,2.5,2.9,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REMPLACER",{"$nulls":6},"9 OPZS SOLAR POWER 1370","HOPPECKE",23,46,2,1370,45,20,78,null,50.9,27,29,null,null,null,"Bon Etat","Bon Etat","Mauvais Etat","Mauvais Etat",2.7,2.7,2.6,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REMPLACER",{"$nulls":5},"Bon","GREEN POWER GENERATORS","01/01/2013","Fonctionnel",null,33.5,null,50,null,0,31,21,12.2,null,25,230,50,25.5,null,12,"55","GP22","DIN55 SMF","Manuel","Non",null,"Oui",1,20,1,"Non",null,null,null,5.0599999999999996,2,11,"CANADIAN SOLAR","CS6P - 230P","Poly",230,7.78,29.6,36.799999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},946,"13:30",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":8},2,null,6,4,null,550,29,"3*35",null,"TOUTES LES MATERIAUX DOIVENT ETRE RECHANGER",6,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,30,null,20,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",0,0,2,0,"Oui",null,"LOCAL BATTRIE","Non"]
["D14","1422010401700","13/07/2020","SEDHIOU","BOUNKELING","NDIAMALATHIEL","KANICOUNDA",76,900,2019,"01/01/2014","01/03/2020",0,"Sud Solar System","ERSEN II",18,6,4,4,32,"BOCAR DIOP",776995764,null,"Non","Non",15000,"Non",414443,1467310,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Bon Etat",null,64,null,null,null,7.8,7.5,"Oui","Bon état",null,"Mauvais état","A remplacer","Bon état",null,"Bon état",null,"Bon état",null,"A réparer",null,null,"LOCAUX ONDULEURS BATTRIE ET GE",null,null,null,"LOCAL GE",2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A Remplacer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"A RESTAURER",{"$nulls":4},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL - 20",1,5,1,5,{"$nulls":10},41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",4,null,null,4.3,2.5,3,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A RESTAURER",{"$nulls":6},"9 OPZS SOLAR POWER 1370","HOPPECKE",21,42,2,1370,45,20,null,null,40.5,{"$nulls":5},"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.5,2.8,"Bon Etat",null,"Mauvais Etat","A remplacer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REMPLACER","A RESTAURER",{"$nulls":4},"Bon","GREEN POWER GENERATOR","01/01/2014",null,null,159.1,null,null,null,0,21,null,12.9,75,25,230,50,255,null,12,"75","GP 22","DIN 75","Manuel","Non",null,"Oui",1,20,30,"Non",null,null,null,5.0599999999999996,2,11,"CANADIAN SOLAR","CS6P - 230P","Poly",230,7.78,29.6,36,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},623,"16:00",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":10},2,9,40,400,32,"3*35",null,"TOUTE L'EQUIPEMENT DOIT ETRE RENOVER",4,null,2,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":10},"Non","Non","Non","Non","Non","Non",0,0,24,0,"Oui",null,null,"Non"]
["D15","1422010300100","13/07/2020","SEDHIOU","BOUNKELING","Djinani","BADIOCOUNDA",51,600,2019,"01/01/2012","01/05/2020",0,"Sud Solar System","ERSEN II",5,1,16,1,23,"OUSMANE CAMARA",779178687,"ARABE","Non","Oui",10000,"Non",414443,1467313,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,18,18,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer",36,5,"Serrure",null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"A réparer",null,"A réparer",null,null,"LOCAUX BATTRI ET GE","LOCAUX ONDULEURS  ET BATTRIE",null,"LOCAL BATTRIE","LOCAL BATTRIE",2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":8},"SERRURE A CHANGER",null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8.OH - 12","SB 5000TL - 20",1,6,1,5,{"$nulls":10},41,63,175,440,26,120,20,22,202,253,108,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",2,null,null,3.8,2.7,2.6,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Bon Etat",{"$nulls":4},"A REFAIRE","SERRURE A REMPLACER",null,"A REFAIRE","A REFAIRE",null,null,"9OPZS SOLAR. POWER 1370","HOPPECKE",23,46,2,1370,45,20,{"$nulls":5},"Bas",null,null,"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",2.7,2.7,2.6,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REMPLACER",{"$nulls":5},"Mauvais","GREEN POWER GENERATIOR","01/01/2012","Non Fonctionnel",{"$nulls":10},25,230,50,25.5,null,12,"75","GP 22","DIN75","Manuel","Non",null,"Oui",1,20,1,"Non",null,null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,1,{"$nulls":8},"LBC","Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":9},1,3,3,42,80,13,"3*35",null,null,3,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",1,0,24,1,"Oui",null,"NEANT","Non"]
["D16","1422010301000","14/07/2020","SEDHIOU","BOUNKELING","Djinani","GASSEKOU",53,420,2019,"01/01/2012","01/06/2020",0,"Sud Solar System","ERSEN II",9,11,8,1,29,"SYLLA FADERA",776733033,"3EM SECONDAIRE","Non","Non",10000,"Oui",416988,1465998,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A remplacer",25.6,10,null,null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"LOCAL BATTRIE","LOCAUX BATTRIES ET ONDULEURS",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":8},"SERRURE A CHANGER",null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8.OH - 12","SB 5000TL - 20",1,6,1,5,47.9,266,3.2,3.1,230,203,50,50,9,9,41,63,175,440,26,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/01/2018",null,4,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REFAIRE","SERRURE A CHANGER",{"$nulls":5},"10 OPZS 1000","HOPPECKE",20,40,2,1000,45,20,{"$nulls":5},"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.5,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GENERATOR",null,"Fonctionnel",null,null,null,52.8,243,null,null,null,12.2,null,25,230,50,25.5,null,12,"75","GP 22","DIN75","Manuel","Non",null,"Oui",1,30,1,"Non",{"$nulls":4},2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"A remplacer",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,2,{"$nulls":4},373,"09:50",null,null,"LBC","Bon",null,"Bon",null,"A réparer",null,"A réparer",{"$nulls":9},1,3,3,50,900,27,"3*35",null,"TOITURES DES LOCAUX A RENOVER",6,1,1,1,1,"Oui","Oui","Non","Oui","Oui","Conducteur",null,null,"Sous traitant",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,30,25,1,25,10,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Sous traitant",null,null,"Conducteur",null,null,72,72,72,72,24,"Non","Non","Non","Non","Non","Non",2,null,24,null,"Oui","LOCAL BATTRIE","NEANT","Non"]
["D17","1422010102300","14/07/2020","SEDHIOU","BOUNKELING","BOGHAL","NDIOLOFENE",80,2204,2019,"01/01/2012","01/01/2017",0,"Sud Solar System","ERSEN II",34,20,10,5,69,"MAMADOU CISSE",771334078,"ARABE","Non","Non",null,null,430587,1459170,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",70,10,null,null,7.5,5.8,"Oui","Bon état",null,"Mauvais état","A réparer","A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,"LOCAUX ONDULEURS ET BATTRIES","LOCAUX ONDULEURS ET BATTRIES",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":6},"REPARER L'ETANCHEITE DE LA TOITURE","SERRURE A REMPLACER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI8.OH - 12","SB 5000TL - 20",2,12,2,10,{"$nulls":10},41,63,175,440,26,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Non",null,"01/01/2017",null,4.2,2.5,3,"Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"REPARER L'ETANCHEITE","SERRURE A REMPLACER",{"$nulls":5},"10 OPZS 1000","HOPPECKE",24,48,2,1000,45,20,{"$nulls":5},"Bas",null,null,"Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.5,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"GREEN POWERGENERATOR","01/01/2012","Non Fonctionnel",{"$nulls":10},25,230,50,25.5,null,null,null,"GP 22",null,"Manuel","Non",null,"Non",{"$nulls":7},7.69,2,12,"REC SOLAR","CS6P - 23OP","Poly",230,7.78,29.6,36.799999999999997,8.4,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},473,"12:45",null,"Bois","LBC","Bon",null,"A réparer",null,"A remplacer",null,"Bon",{"$nulls":7},1,null,1,6,3,45,1500,25,"3*35",null,null,4,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,1,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",{"$nulls":4},"Non",null,null,"Non"]
["D18","1422030102000","14/07/2020","SEDHIOU","BOUNKELING","DIAROUME","KIMBOUTO",36,400,2019,"01/01/2014","01/01/2018",0,"NS RESIF","ERSEN II",3,2,10,2,17,"LAMINE DRAME",782340037,"ARABE","Non","Non",10000,"Oui",441085,1440368,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A remplacer",25,6,null,null,7.5,5.8,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Bon état",null,"Bon état",null,null,null,"LOCAUX ONDULEURS BATTRIES",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"SERRURE A CHANGER",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 500TL - 20",1,5,1,5,{"$nulls":10},41,63,175,440,21,120,20,22,20,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Fonctionnel",null,"Oui",3,null,null,4.2,2.5,3,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":5},"SERRURE A CHANGER",{"$nulls":5},"10 OPZS 1000","HOPPECKE",19,38,2,1000,45,20,{"$nulls":8},"Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GENERATOR","01/01/2014","Non Fonctionnel",{"$nulls":10},25,230,50,25.5,null,12,"70","GP 22","5700185MF","Manuel","Non",null,"Non",{"$nulls":7},5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.5,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},196,"18:06",null,null,null,"Bon",null,"Bon",null,"Bon",null,"A réparer",{"$nulls":8},1,null,5,0,40,50,10,"3*35",null,null,8,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,1,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",0,0,24,1,"Oui","LOCAL BATTRIE","NEANT","Non"]
["D19","1422030100600","14/07/2020","SEDHIOU","BOUNKELING","DIAROUME","BANTANTO",46,600,2019,"NMS","NMS",0,"NS RESIF","ERSEN II",{"$nulls":12},439880,1440219,"Solaire_GE","Non","Non Inondable","Délibération","Oui",{"$nulls":13},"Bon Etat",{"$nulls":5},7.5,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":10},"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":47},"Fonctionnel",null,"Fonctionnel",null,"Non",null,null,null,4,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":34},"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"CUMMINS POWER GENERATOR",{"$nulls":11},22,400,50,{"$nulls":54},"LBC","A réparer",null,"A réparer",null,"Bon",null,"Bon",{"$nulls":10},6,null,40,150,28,"3*35"]
["D20","1422020202000","15/07/2020","SEDHIOU","BOUNKELING","DIACOUNDA","NIOROKI",40,10002,2019,"01/01/2012",0,8,"NS RESIF","ERSEN II",13,7,7,2,29,"SOULEYMANE DIEME",779872484,"ARABE","Non","Oui",10000,"Non",439883,1440229,"Solaire_GE","Oui","Non Inondable","Délibération","Oui",18,18,17,17,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A remplacer","Mauvais Etat","A réparer",70,4,null,null,7.5,5.8,"Oui","A réparer",null,"Mauvais état","A remplacer","Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",{"$nulls":7},2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 8.OH -12","SB 5000TL - 20",1,5,1,5,47.5,299,6.1,11,232,232,50,50,10,10,41,63,175,440,26,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,"01/01/2019",null,4.2,4.2,3,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,null,null,"FISSURE","ETANCHEITE",null,null,"A REPRENDRE",null,null,null,"10 OPZS 1000","HOPPECKE",21,42,2,1000,45,20,null,null,47.5,27,null,null,"01/01/2019","09:50","Bon Etat","Bon Etat","Bon Etat","Bon Etat",2.7,2.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Bon","GREEN POWER GENERATOR","01/01/2012","Non Fonctionnel",{"$nulls":10},25,230,50,25.5,null,null,null,"GP 22",null,"Manuel","Non",null,"Oui",1,20,1,"Non",null,null,null,5.16,2,12,"REC SOLAR","REC 215 AE","Poly",215,7.7,28.2,36.299999999999997,8.3000000000000007,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},640,"10:15",null,"Bois","LBC","Bon",null,"Bon",null,"A réparer",null,"Bon",{"$nulls":9},1,0,8,40,250,33,"3*35",null,"LA BATTRIE DU GE ETAIT EN CHARGE HOR DU VILLAGE L'OR DE LA VISITE",4,0,0,0,0,"Oui","Oui","Non","Oui","Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,30,null,20,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",null,null,3,null,"Oui","LOCAL BATTRIE","NEANT","Non"]
["D21","1432030400200","16/07/2020","SEDHIOU","GOUDOMP","DIOUBOUDOU","BISSARY",36,800,2019,"01/01/2014","01/05/2020",0,"Faye Solaire_Sud Energie","ERSEN II",22,10,7,2,41,"MOUSTAPHA CAMARA",784793643,"ARABE","Non","Non",20000,"Oui",447838,1400270,"Solaire_GE","Non","Non Inondable","Délibération","Oui",18,18,16,18,2,null,"Oui","Grillage","Fer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,15,null,"Autre","POTEAU SUPPORT PORTE",7.2,5.8,"Oui","A réparer",null,"Mauvais état","A réparer","A réparer",null,"A réparer",null,"Bon état",null,"A réparer",null,"LOCAL BATTRIE","LOCAL BATTRIE ET LOCAL GE","LOCAUX ONDULEURS ET BATTRIES",null,null,null,2.7,2.5,3,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":7},"REMPLACER LA SERRUE",null,null,null,"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL - 21",1,null,1,null,47.1,290,5.3,10.4,231,231,50,50,9,9,41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Fonctionnel",null,"Fonctionnel",null,"Oui",4,null,null,4.2,2.5,3,"Mauvais Etat","A réparer","Mauvais Etat","A réparer","Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",null,null,null,"A RESTAURER","A REPRENDRE","SERRURE A CHANGER",{"$nulls":5},"9OPZS SOLAR- POWER","HOPPECKE",20,40,2,1370,45,20,23,124,45.8,27,31,"Bas",null,"10:20","Bon Etat","Bon Etat","Bon Etat","Mauvais Etat",2.7,2.7,2.6,"Bon Etat",null,"Mauvais Etat","A remplacer","A réparer",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A RESTAURER",{"$nulls":5},"Bon","GREEN POWER GENERATOR","01/01/2014","Non Fonctionnel",null,153.4,null,null,null,0,28,6,13.6,null,30,230,50,30.5,null,null,null,"GP 22",null,"Manuel","Non",null,"Oui",0.5,20,null,"Non","2",null,null,5.6,2,11,"CANADIAN SOLAR","CS6P - 230P","Poly",230,7.78,29.6,36.799999999999997,8.34,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":6},538,"10:06",null,"Bois","LBC","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":10},6,0,40,0,22,"3*35",null,null,8,null,5,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",0,0,5,1,"Oui","NEANT","LOCAL BATTRIE","Non",null,"PAR FAUTE DE REPONDANT IL YA CERTAINES RUBRIQUE QUI N'ONT PAS ETRE RENSEIGNER: C'EST LE VOLET MEINTENANCE DES EQUIPEMENTS ET GESTION DES DECHETS"]
["D22","1432020201000","15/07/2020","SEDHIOU","GOUDOMP","KOLIBANTANG","MAKA",99,1200,2019,"01/01/2003","01/01/2016",0,"NS RESIF","ERSEN I",1,3,1,8,13,"MOUSSA SOUWANE",772775275,"ARABE","Non","Non",10000,"Oui",469070,1420894,"Solaire_GE","Non","Non Inondable","Délibération","Oui",19.5,19.5,16,16,3,null,"Non","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Mauvais Etat","A remplacer",31,1,null,null,5.8,5.8,"Oui","Mauvais état",null,"Bon état",null,"A réparer",null,"Bon état",null,"A remplacer",null,"A réparer",null,"C.F LOCAL BATTRIE",null,"C.F LOCAUX ONDULEURS ET BATTRIE",null,"C.F LOCALE BATTRIE","C.F LOCAUX ONDULEURS ET BATTRIES",2.4500000000000002,1.7,2.75,"Bon Etat",null,"A réparer",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"A réparer",null,"Bon Etat",null,"Bon Etat",{"$nulls":4},"A REPRENDRE",null,null,"SERRURE A CHANGER",null,null,null,"Onduleur Chargeur",null,"Monophasé",null,"HP- COMPACT 6000 - 48","RECUPERE PAR L'OPERATEUR",1,5,0,{"$nulls":11},38,68,null,null,null,30,null,null,230,253,null,null,49.95,50.05,null,null,"A remplacer",null,"A remplacer",null,"Non",null,null,null,3.45,2.7,2.8,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Mauvais Etat","A réparer","Bon Etat",null,null,null,"FISSURE A REPARER",null,"SERRURE A REMPLACER",null,"REPRENDRE LA PEINTURE",null,null,null,"8 OPZS 800","HOPPECKE",24,48,2,800,45,20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",2.7,1.9,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Mauvais","CUMMINS POWER GENERATOR","01/01/2003","Non Fonctionnel","01/01/2017",{"$nulls":9},11,400,50,{"$nulls":4},"C 11D5",null,"Manuel","Non",null,"Oui",null,20,1,"Non",null,null,null,5.4,3,12,"ET SOLAR","ET - P636140","Poly",140,7.95,17.600000000000001,21.96,8.41,"Bon",null,"Bon",null,"Bon",null,"A réparer",null,"Bon",null,"A réparer",null,"A remplacer",null,"Bon",null,2,{"$nulls":4},960,"15:00",null,"Bois","LBC","A réparer",null,"A réparer",null,"A remplacer",null,"Bon",null,400,{"$nulls":5},8,null,1,10,0,50,2200,22,"3*35",null,"ONDULEUR DEPOSE PAR L'OPERATEUR ET VOL DE MODULE",3,null,1,{"$nulls":7},"Conducteur",null,null,"Opérateur",null,null,"Conducteur",null,null,"Opérateur",null,null,"Opérateur",null,null,1,null,1,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",2,2,24,1,"Oui","LOCAL BATTRIE","NEANT","Non"]
["D23","0622030300300","18/07/2020","KAOLACK","NIORO","WACK NGOUNA","DAROU MATAR",112,1650,2019,"01/01/2008","2020-01-01",0,"Energie R","ERSEN I",{"$nulls":5},"MODOU FAYE",706530365,null,"Non","Non",{"$nulls":4},"Solaire_GE","Non","Non Inondable","Non Immatriculé","Oui",21,21,15,15,2,null,"Oui","Grillage","Fer",null,null,"Bon Etat",null,"Bon Etat",{"$nulls":5},5.9,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Bon état",{"$nulls":7},2.4,1.6,2.7,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,null,null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL - 20",1,5,1,5,{"$nulls":10},41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Non",null,null,null,4,2.5,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"8 OPZS 800","HOPPECKE",24,48,2,800,45,20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",3.2,1.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Mauvais","CUMMINS POWER GENERATOR",null,"Non Fonctionnel",{"$nulls":10},22,400,50,{"$nulls":4},"C 22 DS",{"$nulls":12},5.0999999999999996,2,15,"SCHOTT SOLAR","ASE - 165 - GT - FI - /MCI","Poly",170,4.78,35.5,44,5.3,"Bon",null,"Bon",null,"A remplacer",null,"Mauvais",null,null,null,"A réparer",null,"A remplacer",null,"Bon",null,4,{"$nulls":7},"Bois","LBC",{"$nulls":24},"ARRET COMPLETE DE LA CENTRALE DEPUIS 2011 C'EST LA SENELEC QUI ALIMENTE LE VILLAGE RECEMMENT DEPUIS 2020",{"$nulls":50},"Non","Non","Non","Non","Non","Non",4,null,24,1]
["D24","0632010201300","18/07/2020","KAOLACK","GUINGUINEO","NDIAGO","NGARE KEUR AMADOU YACINE",58,1361,2019,"01/01/2009","01/01/2017",0,"NS RESIF","ERSEN I",12,11,null,3,26,"ABDOULAYE GUEYE",777046453,"ARABE","Non","Non",10000,"Non",405996,1576726,"Solaire_GE","Non","Inondable","Délibération","Oui",20,20,15,15,2,null,"Oui","Grillage","Fer","Mauvais Etat","A remplacer","Mauvais Etat","A réparer","Bon Etat",null,14,null,null,null,5.8,5.8,"Oui","Bon état",null,"Bon état",null,"Bon état",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",{"$nulls":6},"C.F LOCAL ONDULEUR",2.5,1.7,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A Remplacer",{"$nulls":8},"A FAIRE",null,"Onduleur Chargeur",null,"Monophasé","Monophasé","HP - COMPACT 6000 - 48",null,1,5,{"$nulls":12},38,68,null,null,1,30,null,null,230,253,null,null,49.95,50.05,null,null,"A remplacer",null,"A remplacer",null,"Oui",2,"01/01/2011",null,3.4,2.5,2.9,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":17},"8 OPZS 800","HOPPECKE",24,48,2,800,45,20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",2.7,2,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":10},"Mauvais","COMMINS POWER GENERATION","01/01/2009","Non Fonctionnel","01/01/2017",{"$nulls":9},11,400,50,{"$nulls":4},"C 11D5",null,"Automatique","Non",null,"Oui",null,100,1,"Non",null,null,null,5.0999999999999996,2,15,"SCHOTT SOLAR","ASE - 166 - GT- FI/MCI","Poly",170,4.71,36,44,5.25,"Bon",null,"Bon",null,"Bon",null,"Mauvais",null,"Mauvais",null,"A réparer",null,"A remplacer",null,"Bon",{"$nulls":6},638,"10:05",null,"Bois","LBC","Bon",null,"Bon",null,"A remplacer","A réparer","A remplacer",{"$nulls":7},2,1,1,0,7,40,500,27,"3*35",null,"CENTRALE EN PANNE DEPUIS 2016",8,null,1,null,null,"Oui",null,"Non",null,"Oui","Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,30,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",0,2,24,1,"Oui","LOCAL BATTRIE","NEANT","Non"]
["D25","0622030301200","19/07/2020","KAOLACK","NIORO","WACK NGOUNA","NDIMBA",402,1120,2019,"01/01/2009","01/01/2015",0,"Energie R","ERSEN I",13,13,3,8,37,"ABDOULAYE CISSE",703569828,"ARABE","Non","Non",null,null,384020,1513737,"Solaire_GE","Non","Non Inondable","Délibération","Oui",20,20,16,16,2,null,"Oui","Grillage","Fer","Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,10,null,null,null,5.8,5.8,"Oui","Bon état",null,"Bon état",null,"A réparer",null,"Bon état",null,"Mauvais état","A remplacer","Bon état",null,null,null,"C.F LOCAUX BATTRIES GE",null,"LOCALBATTRIES",null,2.5,1.7,2.8,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",{"$nulls":11},"Onduleur Chargeur","Onduleur Réseau","Monophasé","Monophasé","SI 5048","SB 5000TL - 20",1,5,1,5,{"$nulls":10},41,63,175,440,21,120,20,22,202,253,180,280,45,65,45,65,"Non Fonctionnel",null,"Non Fonctionnel",null,"Oui",2,"01/01/2010","01/01/2010",4,2.5,2.8,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",null,"Mauvais Etat","A Remplacer","Bon Etat",null,"Bon Etat",{"$nulls":5},"SERRURE A REMPLACER",null,"A REFAIRE",null,null,null,"8 OPZS 800","HOPPECKE",24,48,2,800,45,20,{"$nulls":8},"Mauvais Etat","Mauvais Etat","Mauvais Etat","Mauvais Etat",3.2,1.7,2.6,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Bon Etat",null,"Mauvais Etat","A réparer","Bon Etat",{"$nulls":7},"SERRURE A REMPLACER",null,null,"Mauvais","COMMINS POWER GENERATION","01/01/2009","Non Fonctionnel","01/01/2011",{"$nulls":9},22,400,50,{"$nulls":4},"C 22 D5",null,"Automatique","Non",null,"Oui",1,40,null,"Non",null,null,null,5.0999999999999996,2,15,"SCHOTT SOLAR","ASE - 165-GT-FT/MCI","Poly",170,4.78,35.5,44,5.3,"Bon",null,"Bon",null,"Bon",null,"Mauvais","A remplacer","Bon",null,"A réparer",null,"A remplacer",null,"A réparer",{"$nulls":6},960,"11:30",null,null,"LBC","A réparer",null,"A réparer",null,"A réparer",null,"A réparer",null,200,null,5,null,null,null,2,3,3,null,6,40,600,24,"3*35",null,"ARRET COMPLETE DE LA CENTRALE DEPUIS 2015",4,null,1,null,null,"Oui",null,"Oui",null,null,"Conducteur",null,null,"Opérateur",null,null,"Conducteur","Opérateur",null,"Opérateur",null,null,"Opérateur",null,null,1,null,30,null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",null,null,"Opérateur",{"$nulls":7},"Non","Non","Non","Non","Non","Non",null,null,24,1,"Oui","LOCAL BATTRIE","NEANT","Non"]
["M1","WOP","15/07/2020","MATAM","RANEROU","OUDALAYE","WOPPA",57,307,2020,null,"NMS",0,"NEANT","UE FACILITY 2",0,0,0,0,0,"MODOU DEMBA SOW",775785566,{"$nulls":8},"Non",{"$nulls":35},"Bon état",{"$nulls":10},"Bon Etat",{"$nulls":61},"Fonctionnel",null,"Non",{"$nulls":143},"Bois","LED","Bon",null,"Bon",null,"Bon",null,"Bon",{"$nulls":12},45,null,112,"3*35","4*16"]
[]
[]
[]
[]
[]
[]
[{"$nulls":12},"*"]